;*******************************************************************************
; Copyright 2001-2011 Broadcom Corporation.
;
; INF for 64-bit AMD platform (Net server 2003).
;
; InfVersion   15.2.0.4A
;
;*******************************************************************************


[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile = b57amd64.cat
Provider    = %BRCM%
DriverVer   = 05/24/2012,15.2.0.4


[Manufacturer]
%BRCM% = Broadcom, NTamd64, NTamd64.6.0

[ControlFlags]
ExcludeFromSelect = *

[Broadcom]

[Broadcom.NTamd64.6.0]
%BCM5701%           =  BCM5701G.XpInst,          PCI\VEN_14e4&DEV_1645
%BCM5701FA%         =  BCM5701FA.XpInst,         PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_1646
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16a6
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16C6

[Broadcom.NTamd64]
%3C1000BT%          =  3C1000BT.XpInst,          PCI\VEN_14e4&DEV_16A6&SUBSYS_110010B7
%3C1000BT%          =  3C1000BT.XpInst,          PCI\VEN_14e4&DEV_16C6&SUBSYS_110010B7
%3C1000T%           =  3C1000T.XpInst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100710B7
%3C940BR01%         =  3C940BR01.XpInst,         PCI\VEN_14e4&DEV_1645&SUBSYS_100810B7
%3C996BT%           =  3C996BT.XpInst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100610B7
%3C996SX%           =  3C996SX.XpInst,           PCI\VEN_14e4&DEV_1645&SUBSYS_100410B7
%3C998SX%           =  3C998SX.XpInst,           PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C998T%            =  3C998T.XpInst,            PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C999T%            =  3C999T.XpInst,            PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%BCM5701%           =  BCM5701G.XpInst,           PCI\VEN_14e4&DEV_1645
%BCM5701FA%         =  BCM5701FA.XpInst,         PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_1646
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16a6
%BCM5702%           =  BCM5702.XpInst,           PCI\VEN_14e4&DEV_16C6
%BCM5703%           =  BCM5703G.XpInst,           PCI\VEN_14e4&DEV_1647
%BCM5703%           =  BCM5703G.XpInst,           PCI\VEN_14e4&DEV_16a7
%BCM5703%           =  BCM5703G.XpInst,           PCI\VEN_14e4&DEV_16C7
%BCM5703S%          =  BCM5703SW.XpInst,         PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5703S%          =  BCM5703S.XpInst,          PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S.XpInst,          PCI\VEN_14e4&DEV_16a7&SUBSYS_000a14e4
%BCM5703S%          =  BCM5703S.XpInst,          PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5704%           =  BCM5704G.XpInst,           PCI\VEN_14e4&DEV_1648
%BCM5704S%          =  BCM5704S.XpInst,          PCI\VEN_14e4&DEV_16A8
%BCM5704SW%         =  BCM5704SW.XpInst,         PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW%         =  BCM5704SW.XpInst_d,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW%         =  BCM5704SW.XpInst_d,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW%         =  BCM5704SW.XpInst_d,         PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW%         =  BCM5704SW.XpInst_d,         PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014
%BCM5705%           =  BCM5705.XpInst,           PCI\VEN_14e4&DEV_1653
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705F%          =  BCM5705F.XpInst,          PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%          =  BCM5705MA2F2.XpInst,      PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5705M%          =  BCM5705MA2F2.XpInst,      PCI\VEN_14e4&DEV_165E&SUBSYS_127910cf
%BCM5705M%          =  BCM5705MA2F2MFD.XpInst,   PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%          =  BCM5705MA2F2MFD.XpInst,   PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%          =  BCM5705MA2F2MFD.XpInst,   PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033
%BCM5705M%          =  BCM5705MA2.XpInst,        PCI\VEN_14e4&DEV_165E
%BCM5705M%          =  BCM5705MA2.XpInst,        PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5705M%          =  BCM5705MA2.XpInst,        PCI\VEN_14e4&DEV_165E&SUBSYS_0727152d
%BCM5705M%          =  BCM5705M.XpInst,          PCI\VEN_14e4&DEV_165D
%BCM5714%           =  BCM5714G.XpInst,          PCI\VEN_14e4&DEV_1668
%BCM5714%           =  BCM5714.XpInst,           PCI\VEN_14e4&DEV_166A&SUBSYS_03131014
%BCM5714%           =  BCM5780.XpInst,           PCI\VEN_14e4&DEV_166A
%BCM5714%           =  BCM5780.XpInst,           PCI\VEN_14e4&DEV_166A&SUBSYS_107F1734
%BCM5714%           =  BCM5714G.XpInst,          PCI\VEN_14e4&DEV_1678
%BCM5714%           =  BCM5714.XpInst,           PCI\VEN_14e4&DEV_1678&SUBSYS_032a1014
%BCM5714%           =  BCM5714.XpInst,           PCI\VEN_14e4&DEV_1678&SUBSYS_108C1734
%BCM5714S%          =  BCM5714S.XpInst,          PCI\VEN_14e4&DEV_1669
%BCM5714SW%         =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1669&SUBSYS_03281014
%BCM5714SW%         =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1679&SUBSYS_03671014
%BCM5714SW%         =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1669&SUBSYS_03861014
%BCM5714SW%         =  BCM5714SHAL.XpInst,       PCI\VEN_14e4&DEV_1669&SUBSYS_03871014
%BCM5714S%          =  BCM5714S.XpInst,          PCI\VEN_14e4&DEV_166B
%BCM5714S%          =  BCM5714S.XpInst,          PCI\VEN_14e4&DEV_1679
%BCM5714S%          =  BCM5714SWol.XpInst,       PCI\VEN_14e4&DEV_1679&SUBSYS_399710f1
%BCM5722%           =  BCM5750A1G.XpInst,        PCI\VEN_14e4&DEV_165A
%BCM5722%           =  BCM5750A1G.XpInst,        PCI\VEN_14e4&DEV_165A&SUBSYS_02A61028
%BCM5750A1%         =  BCM5750A1F3MEstarDefWolAuto.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%         =  BCM5750A1F3MEstarDefWolAuto.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1%         =  BCM5750A1F3EstarA.XpInst,       PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5750A1%         =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%         =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_167D&SUBSYS_832a1033
%BCM5750A1%         =  BCM5750A1F3MFD.XpInst,       PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%         =  BCM5750A1F3MFD.XpInst,       PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033
%BCM5750A1%         =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1601
%BCM5750A1%         =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_167D
%BCM5750A1%         =  BCM5750A1M.XpInst,        PCI\VEN_14e4&DEV_16FD
%BCM5750A1%         =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_16FF
;%BCM5750A1%        =  BCM5750A1SPECIAL.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_81AA104D
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_5047107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_5048107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0280107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0215107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0460107b
%BCM5750A1%         =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_0604107b
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1658
%BCM5750A1%         =  BCM5750A1G.XpInst,        PCI\VEN_14e4&DEV_1659
%BCM5750A1%         =  BCM5750A1X.XpInst,        PCI\VEN_14e4&DEV_1659&SUBSYS_02c61014
%BCM5750A1%         =  BCM5750A1X.XpInst,        PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014
%BCM5750A1%         =  BCM5750A1X.XpInst,        PCI\VEN_14e4&DEV_1659&SUBSYS_02C61014
%BCM5750A1%         =  BCM5750A1X.XpInst,        PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1676
%BCM5750A1%         =  BCM5750A1eStar.XpInst,    PCI\VEN_14e4&DEV_1677
;%BCM5750A1%        =  BCM5750A1eStar.XpInst,    PCI\VEN_14e4&DEV_1677&SUBSYS_00631025
%BCM5750A1%         =  BCM5750A1eStar.XpInst,    PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014
%BCM5750A1%         =  BCM5750A1eStar.XpInst,    PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%         =  BCM5750A1eStar.XpInst,    PCI\VEN_14e4&DEV_1677&SUBSYS_10961734
%BCM5750A1%         =  BCM5750A1eStar.XpInst,    PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_167C
%BCM5750A1%         =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_16F7
%BCM5750A1%         =  BCM5750MHALeStar.XpInst,       PCI\VEN_14e4&DEV_167D&SUBSYS_05771014
%BCM5750A1%         =  BCM5750MHALeStar.XpInst,       PCI\VEN_14e4&DEV_167D&SUBSYS_208117AA
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%      =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01791028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A71028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01A81028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01AD1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C01028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C11028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CF1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C81028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01C21028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CC1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01D61028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_1600&SUBSYS_01CE1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_019c1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_01E01028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_16F7&SUBSYS_01BF1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01da1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_02311028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_024E1028
%BCM5750A1DMOBILE%  =  BCM5750A1DESTAR.XpInst,  PCI\VEN_14e4&DEV_167B&SUBSYS_01da1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01de1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01e11028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_167A&SUBSYS_01ec1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMOBILE.XpInst,  PCI\VEN_14e4&DEV_1677&SUBSYS_02071028
%BCM5750A1F%        =  BCM5750A1F.XpInst,        PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014
%BCM5750A1F%        =  BCM5750A1F.XpInst,        PCI\VEN_14e4&DEV_167E&SUBSYS_01E41028
%BCM5750A1F%        =  BCM5750A1F.XpInst,        PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01
%BCM5750A1F%        =  BCM5750FHAL.XpInst,       PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014
%BCM5750A1F%        =  BCM5750A1F.XpInst,        PCI\VEN_14e4&DEV_167E
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%           =  BCM5750X.XpInst,          PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_167D&REV_00
%BCM5750%           =  BCM5750.XpInst,           PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01
%BCM5754%           =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1672
%BCM5755%           =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1673
%BCM5750A1DMOBILE%           =  BCM5750A1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1600&SUBSYS_02011028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1672&SUBSYS_02021028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1673&SUBSYS_01f91028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1673&SUBSYS_01fa1028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1673&SUBSYS_01fe1028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1673&SUBSYS_02001028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1673&SUBSYS_024A1028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1673&SUBSYS_01ff1028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1673&SUBSYS_02061028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1672&SUBSYS_01f71028
%BCM5750A1DMOBILE%           =  BCM5750A1DESTAR.XpInst,        PCI\VEN_14e4&DEV_169B&SUBSYS_02201028
%BCM5750A1DMOBILE%           =  BCM5750A1DESTAR.XpInst,        PCI\VEN_14e4&DEV_167A&SUBSYS_021D1028
%BCM5750A1DMOBILE%           =  BCM5750A1DESTAR.XpInst,        PCI\VEN_14e4&DEV_167A&SUBSYS_021E1028
%BCM5750A1DMOBILE%           =  BCM5750A1DESTAR.XpInst,        PCI\VEN_14e4&DEV_167A&SUBSYS_02141028

%BCM5787%           =  BCM5787MA1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_02541028
%BCM5787%           =  BCM5787MA1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_02551028
%BCM5787%           =  BCM5787MA1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_02561028
%BCM5787%           =  BCM5787MA1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_02571028
%BCM5787%           =  BCM5787MA1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_025A1028
%BCM5787%           =  BCM5787MA1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_025B1028
%BCM5787%           =  BCM5787MA1DESTAR.XpInst,        PCI\VEN_14e4&DEV_1693&SUBSYS_02CA1028


%BCM5755%           =  BCM5750A1MeStar.XpInst,        PCI\VEN_14e4&DEV_1674
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1674&SUBSYS_01f81028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1674&SUBSYS_02041028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1674&SUBSYS_02621028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1674&SUBSYS_02631028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1674&SUBSYS_02641028
%BCM5750A1DMOBILE%           =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1674&SUBSYS_02651028

%BCM5755%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167B
%BCM5755%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167B&SUBSYS_10B21734
%BCM5755%           =  BCM5750A1.XpInst,    PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c
%BCM5755%           =  BCM5750A1.XpInst,    PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5755%           =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5755%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_100C17AA
%BCM5755%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_100F17AA
%BCM5755%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_101017AA
%BCM5755%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_101117AA
%BCM5755%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_101317AA
%BCM5755%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_101c17AA
%BCM5755%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_866917AA
%BCM5754%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167A
%BCM5754%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_167A&SUBSYS_10fe1734
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696&SUBSYS_12bb103c
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696&SUBSYS_12bc103c
%BCM5782%           =  BCM5705A2.XpInst,         PCI\VEN_14e4&DEV_1696&SUBSYS_000c103c

%BCM5761%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1680
%BCM5761%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1681

%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_02621028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_02631028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_02641028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_02651028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_02511028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_02DB1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_02EF1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_04281028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_04291028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_04321028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_047B1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1680&SUBSYS_047C1028
%BCM5761%           =  BCM5750A1MeStar_CQ65896.XpInst, PCI\VEN_14e4&DEV_1681&SUBSYS_06691025
%BCM5761%           =  BCM5750A1MeStar_CQ65896.XpInst, PCI\VEN_14e4&DEV_1681&SUBSYS_066B1025
%BCM5761%           =  BCM5750A1MeStar_CQ65896.XpInst, PCI\VEN_14e4&DEV_1681&SUBSYS_07091025
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_02931028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_026D1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_026E1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_02FB1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_04331028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_049A1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_049B1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_04AC1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_04EB1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_04EC1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_053C1028
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_053D1028
%BCM5761_OEM1%      =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1681&SUBSYS_1850103C
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_308217AA
%BCM5750A1DMOBILE%  =  BCM5750A1DMESTAR_CQ47248.XpInst,        PCI\VEN_14e4&DEV_1681&SUBSYS_308217AA

%BCM5761%           =  BCM5761Jumbo.XpInst,            PCI\VEN_14e4&DEV_1680&SUBSYS_300014E4
%BCM5761%           =  BCM5761Jumbo.XpInst,            PCI\VEN_14e4&DEV_1681&SUBSYS_300014E4
%BCM5761%           =  BCM5761Jumbo.XpInst,            PCI\VEN_14e4&DEV_1681&SUBSYS_339C103C
%BCM5761%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1681&SUBSYS_84B81043
%BCM5761%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1681&SUBSYS_1007174B

%BCM5761%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1688
%BCM5761%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1689

%BCM5717%           =  BCM5717.XpInst,                 PCI\VEN_14e4&DEV_1655
%BCM5717%           =  BCM5718.XpInst,                 PCI\VEN_14e4&DEV_1656
%BCM5717%           =  BCM5718_OEM1.XpInst,            PCI\VEN_14e4&DEV_1656&SUBSYS_30451054
%BCM5717%           =  BCM5718_OEM1.XpInst,            PCI\VEN_14e4&DEV_1656&SUBSYS_30461054
%BCM5717%           =  BCM5718_OEM1.XpInst,            PCI\VEN_14e4&DEV_1656&SUBSYS_30471054
%BCM5717%           =  BCM5718_OEM1.XpInst,            PCI\VEN_14e4&DEV_1656&SUBSYS_30521054
%BCM5717%           =  BCM5718_OEM1.XpInst,            PCI\VEN_14e4&DEV_1656&SUBSYS_306C1054
%BCM5717%           =  BCM5718_OEM2.XpInst,            PCI\VEN_14e4&DEV_1656&SUBSYS_80071BCF
%BCM5717%           =  BCM5718_OEM1.XpInst,            PCI\VEN_14e4&DEV_1656&SUBSYS_01801374
%BCM5717%           =  BCM5718S.XpInst,                PCI\VEN_14e4&DEV_1656&SUBSYS_041B1014
%BCM5717%           =  BCM5718S.XpInst,                PCI\VEN_14e4&DEV_1656&SUBSYS_04311014
%BCM5717%           =  BCM5718S.XpInst,                PCI\VEN_14e4&DEV_1656&SUBSYS_180414E4
%BCM5717%           =  BCM5718S.XpInst,                PCI\VEN_14e4&DEV_1656&SUBSYS_180514E4
%BCM5717%           =  BCM5718S.XpInst,                PCI\VEN_14e4&DEV_1656&SUBSYS_280414E4
%BCM5717%           =  BCM5718S.XpInst,                PCI\VEN_14e4&DEV_1656&SUBSYS_280514E4
%BCM5717%           =  BCM5718S_OEM1.XpInst,           PCI\VEN_14e4&DEV_1656&SUBSYS_30681054
%BCM5718_OEM1%      =  BCM5718S.XpInst,                PCI\VEN_14e4&DEV_1656&SUBSYS_4D011186

%BCM5719%           =  BCM5719.XpInst,                 PCI\VEN_14e4&DEV_1657
%BCM5719%           =  BCM5719C_OEM1.XpInst,           PCI\VEN_14e4&DEV_1657&SUBSYS_30471054
%BCM5719%           =  BCM5719C_OEM1.XpInst,           PCI\VEN_14e4&DEV_1657&SUBSYS_30551054
%BCM5719%           =  BCM5719C_OEM1.XpInst,           PCI\VEN_14e4&DEV_1657&SUBSYS_30561054
%BCM5719%           =  BCM5719C_OEM1.XpInst,           PCI\VEN_14e4&DEV_1657&SUBSYS_01801374
%BCM5719%           =  BCM5719C.XpInst,                PCI\VEN_14e4&DEV_1657&SUBSYS_190414E4
%BCM5719%           =  BCM5719S.XpInst,                PCI\VEN_14e4&DEV_1657&SUBSYS_190514E4
%BCM5718S%          =  BCM5719S.XpInst,                PCI\VEN_14e4&DEV_1657&SUBSYS_198014E4
%BCM5719%           =  BCM5719A0.XpInst,               PCI\VEN_14e4&DEV_1657&REV_00
%BCM5719%           =  BCM5719A0C.XpInst,              PCI\VEN_14e4&DEV_1657&SUBSYS_190414E4&REV_00
%BCM5719%           =  BCM5719A0S.XpInst,              PCI\VEN_14e4&DEV_1657&SUBSYS_190514E4&REV_00
%BCM5718S%          =  BCM5719A0S.XpInst,              PCI\VEN_14e4&DEV_1657&SUBSYS_198014E4&REV_00

%BCM5720%           =  BCM5720.XpInst,                 PCI\VEN_14e4&DEV_165F
%BCM5720%           =  BCM5720C.XpInst,                PCI\VEN_14e4&DEV_165F&SUBSYS_200314E4
%BCM5720%           =  BCM5720C.XpInst,                PCI\VEN_14e4&DEV_165F&SUBSYS_1F5B1028
%BCM5720%           =  BCM5720S.XpInst,                PCI\VEN_14e4&DEV_165F&SUBSYS_04DC1028
%BCM5718S%          =  BCM5720S.XpInst,                PCI\VEN_14e4&DEV_165F&SUBSYS_208014E4

%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01391025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_013B1025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_013C1025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_013D1025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01421025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01431025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01451025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01471025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01481025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01491025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_014A1025
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_014B1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01601025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_01611025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_019C1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_019D1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_019E1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_019F1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02001025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02011025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02021025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02031025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02041025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02051025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02061025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02071025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02081025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02091025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_020A1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_020B1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_020C1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_020D1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_020E1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_020F1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02101025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02111025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02121025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02131025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02141025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02151025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02161025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02191025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_021A1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_021B1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_021C1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_021D1025
%BCM5764%           =  BCM5764_CQ35234.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_02211025

%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_0173107B
%BCM5764%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1684&SUBSYS_0174107B

%BCM5750A1DMOBILE%  =  BCM5764DMESTAR.XpInst,          PCI\VEN_14e4&DEV_1684&SUBSYS_02811028
%BCM5750A1DMOBILE%  =  BCM5764DMESTAR.XpInst,          PCI\VEN_14e4&DEV_1684&SUBSYS_02C31028
%BCM5750A1DMOBILE%  =  BCM5764DMESTAR.XpInst,          PCI\VEN_14e4&DEV_1684&SUBSYS_02D61028

%BCM5764%           =  BCM5750A1MeStarX.XpInst,        PCI\VEN_14e4&DEV_165b

%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_025B1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04031025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04051025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04071025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_040A1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_040B1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04131025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04141025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04151025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04161025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04181025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04191025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_041B1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04241025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04251025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_042A1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_043F1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04401025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04411025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04491025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_044A1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_044D1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04521025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04531025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_05671025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_05681025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_05691025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_056A1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_056B1025
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_02FB1028
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04611028
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_04A51028
%BCM57760%          =  BCM57760.XpInst,                PCI\VEN_14e4&DEV_1690&SUBSYS_E0001458

%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_05671025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_05681025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_056B1025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_05781025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_05791025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_057A1025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_057B1025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_05801025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_05811025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_058B1025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_058C1025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B0&SUBSYS_06811025
%BCM57765%          =  BCM57765.XpInst,                PCI\VEN_14e4&DEV_16B4

%BCM57766%          =  BCM57766.XpInst,                PCI\VEN_14e4&DEV_1682
%BCM57766%          =  BCM57766.XpInst,                PCI\VEN_14e4&DEV_1686

%BCM5787%           =  BCM5750A1MeStar.XpInst,         PCI\VEN_14e4&DEV_1693
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_011A1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_011B1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_011C1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_011D1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_011E1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_011F1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01211025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01221025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01231025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01241025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01251025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01261025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01271025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01281025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01291025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_012A1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_012B1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_012C1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_012D1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_012E1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_012F1025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01301025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01311025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01341025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01351025
%BCM5787%           =  BCM5750A1BDFS.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_01361025
%BCM5787%           =  BCM5750A1F3MEstarDefWolAuto.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_139910cf
%BCM5787%           =  BCM5750A1F3MMFDCQ29902.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88741033
%BCM5787%           =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88111033
%BCM5787%           =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88121033
%BCM5787%           =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88361033
%BCM5787%           =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88421033
%BCM5787%           =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88611033
%BCM5787%           =  BCM5750A1F3MMFDEstar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88831033
%BCM5787%           =  BCM5750A1F3MMFDeStar_NoLSO.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88921033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88A11033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88A21033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88A51033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88A91033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88B01033
%BCM5787%           =  BCM5750A1F3MMFDeStar.XpInst,      PCI\VEN_14e4&DEV_1693&SUBSYS_88B91033
%BCM5787%           =  BCM5750MHALeStar.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_20D517AA
%BCM5787MKDMNUN%    =  BCM5750MDisableGig.XpInst,       PCI\VEN_14e4&DEV_1693&SUBSYS_305617AA
%BCM5787MKDMNUN%    =  BCM5750MHALeStar.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_386017AA
%BCM5787MKDMNUN%    =  BCM5750MHALeStar.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_3A2317AA
%BCM5787%           =  BCM5750MHALeStar.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_3D7F17AA
%BCM5787%           =  BCM5750MHALeStar.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_3A2617AA
%BCM5786%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169A
%BCM5786%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169A&SUBSYS_101517aa
%BCM5786%           =  BCM5750A1F3EstarA.XpInst,      PCI\VEN_14e4&DEV_169A&SUBSYS_13ee10cf
%BCM5786%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169A&SUBSYS_101f17AA
%BCM5787%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169B
%BCM5787%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169B&SUBSYS_11291734
%BCM5787%           =  BCM5750A1eStar.XpInst,         PCI\VEN_14e4&DEV_169B&SUBSYS_115C1734
%BCM5787%           =  BCM5750A1F3EstarA.XpInst,       PCI\VEN_14e4&DEV_169B&SUBSYS_139810cf
%BCM5787%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_169B&SUBSYS_203017AA
%BCM5787%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_169B&SUBSYS_100D17AA
%BCM5787%           =  BCM5750HALe.XpInst,       PCI\VEN_14e4&DEV_169B&SUBSYS_100E17AA
%BCM5787F%          =  BCM5750A1FeStar.XpInst,        PCI\VEN_14e4&DEV_167F
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c
%BCM5788%           =  BCM5788FJ.XpInst,         PCI\VEN_14e4&DEV_169c&SUBSYS_123c10cf
%BCM5788%           =  BCM5788FJ.XpInst,         PCI\VEN_14e4&DEV_169c&SUBSYS_12f710cf
%BCM5788%           =  BCM5788MFD.XpInst,         PCI\VEN_14e4&DEV_169c&SUBSYS_82fa1033
%BCM5788%           =  BCM5788MFD.XpInst,         PCI\VEN_14e4&DEV_169c&SUBSYS_83011033
%BCM5789%           =  BCM5789FJ.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_099c103c
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101717aa
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101817aa
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101a17aa
%BCM5788%           =  BCM5788.XpInst,           PCI\VEN_14e4&DEV_169c&SUBSYS_101b17aa
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169D
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_16DD
%BCM5789%           =  BCM5789FJ.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_83101033
%BCM5789%           =  BCM5789FJ.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_83321033
%BCM5789%           =  BCM5789FJ.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_833a1033
%BCM5789%           =  BCM5789FJ.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_881b1033
%BCM5789%           =  BCM5789FJ.XpInst,         PCI\VEN_14e4&DEV_169d&SUBSYS_881c1033
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169D&SUBSYS_0280107b
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169D&SUBSYS_100317AA
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169D&SUBSYS_100517AA
%BCM5789%           =  BCM5789.XpInst,           PCI\VEN_14e4&DEV_169D&SUBSYS_060017FF
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170D
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170E
%BCM5901%           =  BCM5901.XpInst,           PCI\VEN_14e4&DEV_170E&SUBSYS_05451014
%BCM5906%           =  BCM5906eStar.XpInst,           PCI\VEN_14e4&DEV_1712
%BCM5906%           =  BCM5906MeStar.XpInst,          PCI\VEN_14e4&DEV_1713
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_386117AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3D7E17AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3C2C17AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_400617AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3A2317AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_3A2A17AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_305617AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_306117AA
%BCM5906%           =  BCM5906MLEN.XpInst,       PCI\VEN_14e4&DEV_1713&SUBSYS_389B17AA
%BCM5906%           =  BCM5906MFJ.XpInst,        PCI\VEN_14e4&DEV_1713&SUBSYS_143410CF
%BCM5906%           =  BCM5906MDESTAR.XpInst,    PCI\VEN_14e4&DEV_1713&SUBSYS_01F31028
%BCM5906%           =  BCM5906MDESTAR.XpInst,    PCI\VEN_14e4&DEV_1713&SUBSYS_02091028
%BCM5906%           =  BCM5906MDESTAR.XpInst,    PCI\VEN_14e4&DEV_1713&SUBSYS_02861028
%BCM5906%           =  BCM5906MDESTAR.XpInst,    PCI\VEN_14e4&DEV_1713&SUBSYS_02271028
%BCM5906%           =  BCM5906MDESTAR.XpInst,    PCI\VEN_14e4&DEV_1713&SUBSYS_02CA1028
%BCM5906%           =  BCM5906MDESTAR.XpInst,    PCI\VEN_14e4&DEV_1713&SUBSYS_02B61028

%OEM1_DEV4%         =  OEM1_DEV4.XpInst,         PCI\VEN_14e4&DEV_16A6&SUBSYS_81261028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165D&SUBSYS_019c1028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165E&SUBSYS_20031028
%OEM1_DEV5%         =  OEM1_DEV5.XpInst,         PCI\VEN_14e4&DEV_165E&SUBSYS_865d1028
;%OEM1_DEV6%        =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1659&SUBSYS_01841028
;%OEM1_DEV6%        =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1659&SUBSYS_01851028
;%OEM1_DEV6%        =  BCM5750A1.XpInst,         PCI\VEN_14e4&DEV_1677&SUBSYS_01801028
%OEM1_DEV6%         =  OEM1_DEV6.XpInst,         PCI\VEN_14e4&DEV_1653&SUBSYS_86531028

;*******************************************************************************
; 64-bit Windows XP Install sections.
;*******************************************************************************
[BCM5701.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5701.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5701G.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.ParamsC
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5701G.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5702.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5702.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog




[BCM5703.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5703.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5703G.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.ParamsC
AddReg          = Xp64AddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5703G.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5704.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp64AddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5704.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5704G.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS, DelReg.ParamsC, DelReg.DpcDirect
AddReg          = Xp64AddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC1G, ParamsWOLNS, ParamsLgSnd, ParamsWireSpeed, DpcDirect
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5704G.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5705.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5705.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5705.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5788.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5788.Params, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5788.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog




[BCM5788FJ.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5788.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL , ParamsLogOptions, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5788FJ.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5788MFD.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5788.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL , ParamsLogOptions, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5788MFD.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog





[BCM5789FJ.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo , DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5788.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL , ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5789FJ.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog





[BCM5789.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo , DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5789.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5750.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShasta, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750X.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShasta, ParamsWireSpeed, ParamsLgSnd, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750X.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1X.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1X.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1G.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.ParamsC
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC1G, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1G.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1eStar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1eStar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1MeStar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1MeStar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1MeStar_CQ65896.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsCQ65896
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1MeStar_CQ65896.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1MeStarX.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1MeStarX.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5764_CQ35234.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsCQ35234
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5764_CQ35234.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5761Jumbo.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSndJumboCombo_5761, ParamsM
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5761Jumbo.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5717.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM5717.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5717.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5718.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM5717.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsEEE, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5718.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5718_OEM1.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM5717_OEM1.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsEEE
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5718_OEM1.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5718_OEM2.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM5717_OEM1.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsEEE
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5718_OEM2.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5718S.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5718S.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5718S.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5718S_OEM1.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5718S_OEM1.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsWOLTbi, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5718S_OEM1.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5719.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE, DelReg.LgSnd_all
AddReg          = Xp64AddReg, BCM5719.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsM, ParamsEEE_CO, ParamsLgSnd, ParamsJumbo, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5719.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5719C.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE, DelReg.LgSnd_all
AddReg          = Xp64AddReg, BCM5719.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsEEE, ParamsLgSnd, ParamsJumbo, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5719C.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5719C_OEM1.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE, DelReg.LgSnd_all
AddReg          = Xp64AddReg, BCM5719_OEM1.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsEEE, ParamsLgSnd, ParamsJumbo, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5719C_OEM1.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5719S.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5719.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5719S.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5719A0.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE, DelReg.LgSnd_all
AddReg          = Xp64AddReg, BCM5719.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed_CO, ParamsM, ParamsEEE_CO, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5719A0.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5719A0C.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE, DelReg.LgSnd_all
AddReg          = Xp64AddReg, BCM5719.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM, ParamsEEE, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5719A0C.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5719A0S.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5719.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsM, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5719A0S.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5720.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM5720.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC_CO, ParamsWOLeStar_CO, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsEEE_CO, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5720.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5720C.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM5720.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsEEE, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5720C.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5720S.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5720.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsWOLTbi_None, ParamsTuning
AddReg          = ParamsRingSize
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5720S.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM57760.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode
AddReg          = Xp64AddReg, BCM57760.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM57760.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM57765.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM57765.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsEEE
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM57765.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM57766.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.GphyGreenMode, DelReg.EEE
AddReg          = Xp64AddReg, BCM57766.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsJumbo, ParamsEEE
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM57766.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5764DMESTAR.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.Jumbo, DelReg.WireSpeed, DelReg.TaskOffload
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xDE, ParamsC, DMobile.Params, ParamsWOLNS, Estar, ParamsM
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5764DMESTAR.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1BDFS.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1BDFS.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5906.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5906.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5906eStar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5906eStar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5906MDESTAR.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd, DelReg.Wol, DelReg.LAA, DelReg.TaskOffload
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xDE, ParamsC100, ParamsWOLNS, 5906DMobile.Params, eStar
CopyFiles       = CopyFile.XpSys64
BusType         = 5
[BCM5906MDESTAR.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5906MLEN.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd, DelReg.Wol
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5906MLEN.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5906MFJ.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5906MFJ.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5714.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5714.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5714G.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic, DelReg.ParamsC
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC1G, ParamsWireSpeed, ParamsLgSndJumboCombo, ParamsWOL, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5714G.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5780.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSndJumboCombo, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5780.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5714S.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsLgSndJumboCombo, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5714S.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5714SWol.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
DelReg          = DelReg.Wol
DelReg          = DelReg.WolMagic
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsWOLTbi, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5714SWol.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5714SHAL.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750R.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsWOLTbi, ParamsDropVlan, IntrCoal, ParamsTuning
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5714SHAL.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1F3.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL , ParamsLgSnd , ParamsWireSpeed , ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1F3Estar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar , ParamsLgSnd , ParamsWireSpeed , ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3Estar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5750A1F3EstarA.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar, ParamsLgSnd , ParamsWireSpeed , ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3EstarA.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5750A1F3MFD.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar , ParamsLgSnd , ParamsWireSpeed , ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3MFD.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog




[BCM5750A1F3M.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar , ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3M.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1F3MEstarDefWolAuto.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLeStar , ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3MEstarDefWolAuto.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5750A1F3MMFD.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLogOptions, ParamsM, ParamsWireSpeed, ParamsLgSnd, ParamsNT
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3MMFD.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1F3MMFDEstar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLEstar , ParamsLogOptions, ParamsM, ParamsWireSpeed, ParamsLgSnd, ParamsNT
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3MMFDEstar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1F3MMFDEstar_NoLSO.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd_all
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLEstar , ParamsLogOptions, ParamsM, ParamsWireSpeed, ParamsNT
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3MMFDEstar_NoLSO.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1F3MMFDCQ29902.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOLEstar , ParamsLogOptions, ParamsM, ParamsCQ29902
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F3MMFDCQ29902.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5750A1M.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsM, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1M.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5906M.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5906M.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5906MeStar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5906MeStar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5906MDMESTAR.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed, DelReg.LgSnd
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, Estar
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5906MDMESTAR.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5750MHAL.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsM,  ParamsWOLLink, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750MHAL.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750MHALeStar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM,  ParamsWOLLink, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750MHALeStar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750MDisableGig.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsM,  ParamsWOLLink, ParamsWireSpeed, ParamsLgSnd, ParamsDisableGig
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750MDisableGig.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750HALe.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar,  ParamsWOLLink, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750HALe.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1F.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1F.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1FeStar.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1FeStar.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog




[BCM5750FHAL.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWOLLink, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750FHAL.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5750A1DMOBILE.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xDE, ParamsC, ParamsWOLNS, DMobile.Params
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1DMOBILE.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1DMESTAR.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.Jumbo, DelReg.WireSpeed, DelReg.TaskOffload
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xDE, ParamsC, DMobile.Params, ParamsWOLNS, Estar, ParamsM
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1DMESTAR.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1DMESTAR_CQ47248.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.Jumbo, DelReg.WireSpeed, DelReg.TaskOffload
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xDE, ParamsC, DMobile.Params, ParamsWOLNS, Estar, ParamsM, ParamsCQ47248
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1DMESTAR_CQ47248.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5750A1DESTAR.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.WireSpeed, DelReg.TaskOffload
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xDE, ParamsC, DMobile.Params, ParamsWOLNS, Estar
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5750A1DESTAR.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5787MA1DESTAR.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.WireSpeed, DelReg.TaskOffload
AddReg          = Xp64AddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xDE, ParamsC, DMobile.Params, ParamsWOLNS, ParamsM, Estar
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5787MA1DESTAR.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5705MA2F2.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp64AddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5705MA2F2.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5705MA2F2MFD.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp64AddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5705MA2F2MFD.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog





[BCM5705M.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5705M.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5705M.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[BCM5705A2.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp64AddReg, BCM5705A2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5705A2.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5705F.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp64AddReg, BCM5705F.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5705F.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5705MA2.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp64AddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5705MA2.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5901.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5901.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5901.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5701FA.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5701FA.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5703S.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol
AddReg          = Xp64AddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5703S.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5703SW.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol
AddReg          = Xp64AddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5703SW.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5704S.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.DpcDirect
AddReg          = Xp64AddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, DpcDirect
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5704S.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[BCM5704SW.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp64AddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5704SW.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog

[BCM5704SW.XpInst_d.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp64AddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi, ParamsDropVlan
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[BCM5704SW.XpInst_d.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[3C996SX.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C996SX.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[3C996BT.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C996BT.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[3C1000T.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C1000T.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[3C940BR01.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C940BR01.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog


[3C998T.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C998T.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[3C998SX.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C998SX.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[3C999T.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C999T.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[3C1000BT.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[3C1000BT.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[OEM1_DEV4.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp64AddReg, BCM5702.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsNtW9xDE, DMobile.Params
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[OEM1_DEV4.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



[OEM1_DEV5.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5705M.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xDE, ParamsC, ParamsWOLNS, DMobile.Params
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[OEM1_DEV5.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog




[OEM1_DEV6.XpInst.NTamd64]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp64AddReg, BCM5705M.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xDE, ParamsC, ParamsWOLNS, DMobile.Params
CopyFiles       = CopyFile.XpSys64
BusType         = 5

[OEM1_DEV6.XpInst.NTamd64.Services]
AddService = b57nd, 2, BCM5701.Xp64AddService, Xp64EventLog



;*******************************************************************************
; 64-bit Windows Xp common sections.
;*******************************************************************************

[Xp64AddReg]
HKR, Ndi,            Service,    0, "b57nd"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Xp64EventLog]
AddReg = Xp64AddEventLogReg

[Xp64AddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57amd64.sys"
HKR, , TypesSupported  , 0x00010001, 7


[BCM5701.Xp64AddService]
DisplayName    = %BCM5701%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57amd64.sys
LoadOrderGroup = NDIS
Addreg         = bcmPnpInstallReg

[bcmPnpInstallReg]
HKR,,product_version,0,"17.2.0"

;*******************************************************************************
; Registry parameters.
;*******************************************************************************

[BCM5701.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5702.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5703.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5704.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705M.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705A2.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705F.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705MA2.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5788.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750R.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5717.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , GphyGreenMode,            0, "4"

[BCM5717_OEM1.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , GphyGreenMode,            0, "4"

[BCM5718S.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5718S_OEM1.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"

[BCM5719.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , Limit4kBd,                0, "1"

[BCM5719_OEM1.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , Limit4kBd,                0, "1"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"

[BCM5720.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM57760.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , GphyGreenMode,            0, "4"

[BCM57765.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"
HKR, , GphyGreenMode,            0, "4"

[BCM57766.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
HKR, , RxMaxCoalescedFramesDuringInt, 0, "0"

[BCM5901.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[DMobile.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1500"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"
HKR, , LargeSendOffload,         0, "1"

[5906DMobile.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1500"


[ParamsNt]
HKR, Ndi\Params\TaskOffloadCap,      ParamDesc, , %TaskOffload%
HKR, Ndi\Params\TaskOffloadCap,      default,   , "63"
HKR, Ndi\Params\TaskOffloadCap,      type,      , "enum"
HKR, Ndi\Params\TaskOffloadCap\enum, 0,         , %TaskOffload_None%
HKR, Ndi\Params\TaskOffloadCap\enum, 42,        , %TaskOffload_Rx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 21,        , %TaskOffload_Tx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 63,        , %TaskOffload_Rx_Tx_Chksum%


[ParamsNtW9xFJ]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "0"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"




[ParamsNt8021p]
HKR, Ndi\Params\Enable8021p,      ParamDesc, , %QOS_8021p%
HKR, Ndi\Params\Enable8021p,      default,   , "0"
HKR, Ndi\Params\Enable8021p,      type,      , "enum"
HKR, Ndi\Params\Enable8021p\enum, 0,         , %QOS_8021p_Disable%
HKR, Ndi\Params\Enable8021p\enum, 1,         , %QOS_8021p_Enable%


[ParamsNtW9x]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsNtW9xDE]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%



[ParamsJumbo]
HKR, Ndi\Params\RxMtu, ParamDesc, , %JumboMtu%
HKR, Ndi\Params\RxMtu, default,   , "1500"
HKR, Ndi\Params\RxMtu, type,      , "dword"
HKR, Ndi\Params\RxMtu, min,       , "1500"
HKR, Ndi\Params\RxMtu, max,       , "9000"
HKR, Ndi\Params\RxMtu, step,      , "500"
HKR, Ndi\Params\RxMtu, base,      , "10"



[ParamsWOLLink]
HKR, Ndi\Params\WakeOnLink,        ParamDesc, , %WakeOnLink%
HKR, Ndi\Params\WakeOnLink,        default,   , "0"
HKR, Ndi\Params\WakeOnLink,        type,      , "enum"
HKR, Ndi\Params\WakeOnLink\enum,   0,         , %WakeOnLink_Disable%
HKR, Ndi\Params\WakeOnLink\enum,   1,         , %WakeOnLink_Enable%




[ParamsLogOptions]
HKR, Ndi\Params\LogLevelInfo,        ParamDesc, , %LogLevelInfo%
HKR, Ndi\Params\LogLevelInfo,        default,   , "0"
HKR, Ndi\Params\LogLevelInfo,        type,      , "enum"
HKR, Ndi\Params\LogLevelInfo\enum,   0,         , %LogLevelInfo_Disable%
HKR, Ndi\Params\LogLevelInfo\enum,   1,         , %LogLevelInfo_Enable%
HKR, Ndi\Params\LogLevelWarn,        ParamDesc, , %LogLevelWarn%
HKR, Ndi\Params\LogLevelWarn,        default,   , "0"
HKR, Ndi\Params\LogLevelWarn,        type,      , "enum"
HKR, Ndi\Params\LogLevelWarn\enum,   0,         , %LogLevelWarn_Disable%
HKR, Ndi\Params\LogLevelWarn\enum,   1,         , %LogLevelWarn_Enable%


[ParamsM]
HKR, , ClockControl,          0, "1"

[ParamsCQ29902]
HKR, , CQ29902Errata,          0, "0"

[ParamsCQ35234]
HKR, , CQ35234,               0, "0"

[ParamsCQ47248]
HKR, , CQ47248,               0, "0"

[ParamsCQ65896]
HKR, , PnPCapabilities,       0, "288"

[ParamsWireSpeed]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsWireSpeed_CO]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed_CO%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%


[ParamsC]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%

[ParamsC_CO]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex_CO%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%


[ParamsC100]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%
[ParamsC1G]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 8200,      , %Speed_Duplex_1000Mb_Fd%


[ParamsWOL]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%


[ParamsWOLeStar]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "256"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,         , %WolSpeed_LowestAvail%

HKR, , WolSpeed,                 0, "256"

[ParamsWOLeStar_CO]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode_CO%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed_CO%
HKR, Ndi\Params\WolSpeed,       default,   , "256"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,         , %WolSpeed_LowestAvail%

HKR, , WolSpeed,                 0, "256"

[Estar]
HKR, , WolSpeed,                 0, "256"

[ParamsWOLeStarDefWolAuto]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,         , %WolSpeed_LowestAvail%
HKR, , WolSpeed,                 0, "0"

[ParamsWOLShasta]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
; HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
; HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
;HKR, Ndi\Params\WolSpeed\enum,  3,         , %WolSpeed_1000mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%

[ParamsWOLTbi]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, , TbiWol,                   0, "1"

[ParamsWOLTbi_None]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "0"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, , TbiWol,                   0, "1"

[ParamsLgSnd]
HKR, Ndi\Params\LargeSendOffload,    ParamDesc, , %TaskOffload_LargeSend%
HKR, Ndi\Params\LargeSendOffload,    default,   , "1"
HKR, Ndi\Params\LargeSendOffload,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffload\enum, 0,        , %TaskOffload_LargeSend_Disable%
HKR, Ndi\Params\LargeSendOffload\enum, 1,        , %TaskOffload_LargeSend_Enable%
HKR, , LargeSendOffload,         0, "1"

[ParamsWOLNS]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%


[ParamsLgSndJumboCombo]
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    ParamDesc, , %TaskOffload_LargeSend_Jumbo%
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    default,   , "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 0,        , %TaskOffload_LargeSend_Disable_Both%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 1,        , %TaskOffload_LargeSend_Enable_JumboDisable%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 2,        , %TaskOffload_LargeSend_Disable_JumboEnable3000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 3,        , %TaskOffload_LargeSend_Disable_JumboEnable4500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 4,        , %TaskOffload_LargeSend_Disable_JumboEnable6000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 5,        , %TaskOffload_LargeSend_Disable_JumboEnable7500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 6,        , %TaskOffload_LargeSend_Disable_JumboEnable9000%

[ParamsLgSndJumboCombo_5761]
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    ParamDesc, , %TaskOffload_LargeSend_Jumbo%
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    default,   , "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 0,        , %TaskOffload_LargeSend_Disable_Both%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 1,        , %TaskOffload_LargeSend_Enable_JumboDisable%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 2,        , %TaskOffload_LargeSend_Disable_JumboEnable3000%

[ParamsDropVlan]
HKR, , DropVlanPkt,          0, "1"

[DpcDirect]
HKR, , ScheduleDpcDirect,     0, "1"

[ParamsRingSize]
HKR, , LargeSizeRxRing,       0, "0"

[IntrCoal]
HKR, Ndi\Params\InterruptModeration,     ParamDesc, 0, %ParamDesc_InterruptModeration%
HKR, Ndi\Params\InterruptModeration,     Type,      0, "enum"
HKR, Ndi\Params\InterruptModeration,     Default,   0, "1"
HKR, Ndi\Params\InterruptModeration,     Optional,  0, "0"
HKR, Ndi\Params\InterruptModeration\enum, "0",      0, "%GenDisable%"
HKR, Ndi\Params\InterruptModeration\enum, "1",      0, "%GenEnable%"

[ParamsTuning]
HKR, Ndi\Params\*ReceiveBuffers,      ParamDesc,        0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,      type,             0, "enum"
HKR, Ndi\Params\*ReceiveBuffers,      Default,          0, "200"
HKR, Ndi\Params\*ReceiveBuffers\enum, "200",            0, %Default%
HKR, Ndi\Params\*ReceiveBuffers\enum, "16",             0, %Minimum%
HKR, Ndi\Params\*ReceiveBuffers\enum, "511",            0, %Maximum%

HKR, Ndi\Params\*TransmitBuffers,   ParamDesc,          0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,   type,               0, "int"
HKR, Ndi\Params\*TransmitBuffers,   default,            0, "200"
HKR, Ndi\Params\*TransmitBuffers,   min,                0, "100"
HKR, Ndi\Params\*TransmitBuffers,   max,                0, "600"

[ParamsEEE]
HKR, Ndi\Params\*EEE,               ParamDesc, , %EEE%
HKR, Ndi\Params\*EEE,               default,   , "0"
HKR, Ndi\Params\*EEE,               type,      , "enum"
HKR, Ndi\Params\*EEE\enum,          0,         , %EEE_Disable%
HKR, Ndi\Params\*EEE\enum,          1,         , %EEE_Enable%
HKR, , *EEE, 0, "0"

HKR, Ndi\Params\EeeCtrlMode,        ParamDesc, , %EEE_Control%
HKR, Ndi\Params\EeeCtrlMode,        default,   , "1"
HKR, Ndi\Params\EeeCtrlMode,        type,      , "enum"
HKR, Ndi\Params\EeeCtrlMode\enum,   0,         , %EEE_MaxPowerSave%
HKR, Ndi\Params\EeeCtrlMode\enum,   1,         , %EEE_Balance%
HKR, Ndi\Params\EeeCtrlMode\enum,   2,         , %EEE_MaxPerformance%

[ParamsEEE_CO]
HKR, Ndi\Params\*EEE,               ParamDesc, , %EEE_CO%
HKR, Ndi\Params\*EEE,               default,   , "0"
HKR, Ndi\Params\*EEE,               type,      , "enum"
HKR, Ndi\Params\*EEE\enum,          0,         , %EEE_Disable%
HKR, Ndi\Params\*EEE\enum,          1,         , %EEE_Enable%
HKR, , *EEE, 0, "0"

HKR, Ndi\Params\EeeCtrlMode,        ParamDesc, , %EEE_Control_CO%
HKR, Ndi\Params\EeeCtrlMode,        default,   , "1"
HKR, Ndi\Params\EeeCtrlMode,        type,      , "enum"
HKR, Ndi\Params\EeeCtrlMode\enum,   0,         , %EEE_MaxPowerSave%
HKR, Ndi\Params\EeeCtrlMode\enum,   1,         , %EEE_Balance%
HKR, Ndi\Params\EeeCtrlMode\enum,   2,         , %EEE_MaxPerformance%


[ParamsDisableGig]
HKR, , DisableGig,               0, "1"

;*******************************************************************************
; Keys to remove.
;*******************************************************************************

[DelReg.RequestedMediaType]
HKR, Ndi\Params\RequestedMediaType

[DelReg.Wol]
HKR, Ndi\Params\WakeUpModeCap
HKR, Ndi\Params\WolSpeed

[DelReg.WolS]
HKR, Ndi\Params\WolSpeed

[DelReg.WolMagic]
HKR, Ndi\Params\WakeUpModeCap
HKR, Ndi\Params\WolSpeed

[DelReg.Jumbo]
HKR, Ndi\Params\RxMtu

[DelReg.GphyGreenMode]
HKR, Ndi\Params\GphyGreenMode

[DelReg.LgSnd]
HKR, Ndi\Params\LargeSendOffload

[DelReg.LgSnd_all]
HKR, Ndi\Params\LargeSendOffload
HKR, ,LargeSendOffload

[DelReg.WireSpeed]
HKR, Ndi\Params\WireSpeed

[DelReg.ClockControl]
HKR, ,ClockControl

[DelReg.LAA]
HKR, Ndi\params\NetworkAddress
HKR, , NetworkAddress

[DelReg.TaskOffload]
HKR, Ndi\Params\TaskOffloadCap

[DelReg.ParamsC]
HKR, Ndi\Params\RequestedMediaType

[DelReg.DpcDirect]
HKR, ,ScheduleDpcDirect

[DelReg.EEE]
HKR, Ndi\Params\EeePhyEnable
HKR, Ndi\Params\EeeCtrlMode
HKR, Ndi\Params\*EEE

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 11
CopyFile.XpSys64 = 12

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
b57amd64.sys = 1

[CopyFile.XpSys64]
b57amd64.sys,,,1



;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
BRCM                = "Broadcom"
DISK_DESC           = "Broadcom NetXtreme Installation Media"

BCM5700FB           = "Broadcom NetXtreme Gigabit Fiber"
BCM5700FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5702             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5703SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5704SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705F            = "Broadcom 570x 10/100 Integrated Controller"
BCM5750            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1        = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1F        = "Broadcom NetXtreme Fast Ethernet"
BCM5714               = "Broadcom NetXtreme Gigabit Ethernet"
BCM5714S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5714SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5722             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1STSP    = "Embedded Broadcom NetXtreme 5721 PCI-E Gigabit NIC"
BCM5750B0           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750B0F          = "Broadcom NetXtreme Fast Ethernet"
BCM5754             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5755             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5782             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5761             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5717             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5718S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5719             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5720             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5764             = "Broadcom NetXtreme Gigabit Ethernet"
BCM57760            = "Broadcom NetXtreme Gigabit Ethernet"
BCM57765            = "Broadcom NetXtreme Gigabit Ethernet"
BCM57766            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5786             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787MKDMNUN      = "Broadcom NetLink (TM) Ethernet"
BCM5787F            = "Broadcom NetLink (TM) Fast Ethernet"
BCM5788             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5789             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5901             = "Broadcom NetXtreme Fast Ethernet"
BCM5906             = "Broadcom NetLink (TM) Fast Ethernet"

BCM5718_OEM1        = "D-Link\DGE-560SX (Fiber mode only)"

3C996T              = "3Com 3C996 10/100/1000 Server NIC"
3C996SX             = "3Com 3C996 Gigabit Fiber-SX Server NIC"
3C996BT             = "3Com 3C996B Gigabit Server NIC"
3C1000T             = "3Com 3C1000 Gigabit NIC"
3C940BR01           = "3Com 3C940 Gigabit LOM"
3C998T              = "3Com Dual Port 10/100/1000 PCI-X Server NIC"
3C998SX             = "3Com Dual Port 1000-SX PCI-X Server NIC"
3C999T              = "3Com Quad Port 10/100/1000 PCI-X Server NIC"
3C1000BT            = "3Com 10/100/1000 PCI"

OEM1_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV4           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV5           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"

OEM2_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM2_DEV2           = "Broadcom NetXtreme Fast Ethernet"
OEM2_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM2_DEV4           = "Broadcom NetXtreme Fast Ethernet"

OEM3_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"

BCM5750A1DSF        = "Broadcom NetXtreme 5751 Gigabit Controller"
BCM5750A1DSSF       = "Broadcom NetXtreme 5721 Gigabit Controller"
BCM5750A1DDT        = "Broadcom NetXtreme 57xx Gigabit Controller"
BCM5750A1DMOBILE    = "Broadcom NetXtreme 57xx Gigabit Controller"

BCM5761_OEM1        = "Broadcom NetXtreme Gigabit Ethernet Plus"

; These items will be set by IHV...
DriverMfgr            = "Broadcom"                  ; IHV name
DriverVersionID       = "5.00"                      ; The IHV driver version
BaseDriverFileVersion = "15.2"
BaseDriverFileName    = "b57amd64.sys"               ; Key file for version

; These items will be set by IHV and updated by OEM
DriverOEM         = "Dell"      ; name of the OEM
DriverFamily      = "NIC"       ; device family (NIC, Storage, Video...)
DriverProduct     = "BCM5700"   ; Specific Name of device (chipset, for example)
DriverDescription = "Broadcom NetXtreme Gigabit Ethernet"  ; Description of device (product name, OS or system supported)
DriverOEMVersion  = "A00"       ; OEM-specified version


JumboMtu = "Jumbo Mtu"

FlowControl             = "Flow Control"
FlowControl_Disable     = "Disable"
FlowControl_Rx_Pause    = "Rx PAUSE"
FlowControl_Tx_Pause    = "Tx PAUSE"
FlowControl_Rx_Tx_Pause = "Rx/Tx PAUSE"
FlowControl_Auto        = "Auto"

Speed_Duplex          = "Speed & Duplex"
Speed_Duplex_CO       = "Speed & Duplex (Copper Only)"
Speed_Duplex_Auto     = "Auto"
Speed_Duplex_10Mb_Hd  = "10 Mb Half"
Speed_Duplex_10Mb_Fd  = "10 Mb Full"
Speed_Duplex_100Mb_Hd = "100 Mb Half"
Speed_Duplex_100Mb_Fd = "100 Mb Full"
Speed_Duplex_1000Mb_Fd = "1 Gb Full Auto"

QOS_8021p         = "802.1p QOS"
QOS_8021p_Disable = "Disable"
QOS_8021p_Enable  = "Enable"

WireSpeed         = "Ethernet@WireSpeed"
WireSpeed_CO      = "Ethernet@WireSpeed (Copper Only)"
WireSpeed_Disable = "Disable"
WireSpeed_Enable  = "Enable"

WakeOnLink         = "Wake On Link"
WakeOnLink_Disable = "Disable"
WakeOnLink_Enable  = "Enable"
TaskOffload              = "Checksum Offload"
TaskOffload_None         = "None"
TaskOffload_Rx_Chksum    = "Rx TCP/IP Checksum"
TaskOffload_Tx_Chksum    = "Tx TCP/IP Checksum"
TaskOffload_Rx_Tx_Chksum = "Tx/Rx TCP/IP Checksum"

TaskOffload_LargeSend           = "Large Send Offload"
TaskOffload_LargeSend_Disable   = "Disable"
TaskOffload_LargeSend_Enable    = "Enable"
`
TaskOffload_LargeSend_Jumbo                           = "LSO & Jumbo Frames"
TaskOffload_LargeSend_Disable_Both                = "Both Disabled"
TaskOffload_LargeSend_Enable_JumboDisable   = "LSO Enabled,Jumbo Off"
TaskOffload_LargeSend_Disable_JumboEnable3000   = "LSO Off,Jumbo 3000"
TaskOffload_LargeSend_Disable_JumboEnable4500   = "LSO Off,Jumbo 4500"
TaskOffload_LargeSend_Disable_JumboEnable6000   = "LSO Off,Jumbo 6000"
TaskOffload_LargeSend_Disable_JumboEnable7500   = "LSO Off,Jumbo 7500"
TaskOffload_LargeSend_Disable_JumboEnable9000   = "LSO Off,Jumbo 9000"

WakeUpMode         = "Wake Up Capabilities"
WakeUpMode_CO      = "Wake Up Capabilities (Copper Only)"
WakeUpMode_None    = "None"
WakeUpMode_Magic   = "Magic Packet"
WakeUpMode_Pattern = "Wake Up Frame"
WakeUpMode_Both    = "Both"

WolSpeed       = "WOL Speed"
WolSpeed_CO    = "WOL Speed (Copper Only)"
WolSpeed_Auto  = "Auto"
WolSpeed_10mb  = "10 Mb"
WolSpeed_100mb = "100 Mb"
WolSpeed_1000mb = "1000 Mb"
WolSpeed_LowestAvail = "Lowest Speed Advertised"

NetworkAddress           = "Locally Administered Address"


LogLevelInfo    = "Log Information Messages"
LogLevelWarn  = "Log Warning Messages"
LogLevelInfo_Disable  =  "Disable"
LogLevelInfo_Enable  =  "Enable"
LogLevelWarn_Disable  =  "Disable"
LogLevelWarn_Enable  =  "Enable"

ParamDesc_InterruptModeration   = "Interrupt Moderation"
ReceiveBuffers  =       "Receive Buffers"
TransmitBuffers =       "Transmit Buffers"

Default   =  "Default"
Minimum   =  "Minimum"
Maximum   =  "Maximum"

;; Interrupt Coalescing Options
;;
GenEnable       = "Enable"
GenDisable      = "Disable"

EEE                     = "802.3az EEE"
EEE_CO                  = "802.3az EEE (Copper Only)"
EEE_Disable             = "Disable"
EEE_Enable              = "Enable"

EEE_Control				= "EEE Control Policies"
EEE_Control_CO		= "EEE Control Policies (Copper Only)"
EEE_MaxPowerSave		= "Maximum Power Saving"
EEE_Balance				= "Optimal Power and Performance"
EEE_MaxPerformance		= "Maximum Performance"
