;*******************************************************************************
; Copyright 2001-2011 Broadcom Corporation.
;
; INF for 32-bit Windows 2K, Windows XP and Windows server 2003
;
; InfVersion   15.2.0.4
;
;*******************************************************************************

[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile = b57win32.cat
Compatible  = 1
Provider    = %BRCM%
DriverVer   = 05/24/2012,15.2.0.4

[Manufacturer]
%BRCM% = Broadcom, NTx86.5.1, NTx86.6.0, NTamd64

[Broadcom.NTamd64]

[Broadcom.NTx86.6.0]
%BCM5700%      =  BCM5700CX.XpInst,   PCI\VEN_14e4&DEV_1644&REV_21
%BCM5700%      =  BCM5700CX.XpInst,   PCI\VEN_14e4&DEV_1644&REV_22
%BCM5700%      =  BCM5700.XpInst,     PCI\VEN_14e4&DEV_1644
%BCM5700FA%    =  BCM5700FA.XpInst,   PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5700FB%    =  BCM5700FB.XpInst,   PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5701%      =  BCM5701.XpInst,     PCI\VEN_14e4&DEV_1645
%BCM5701FA%    =  BCM5701FA.XpInst,   PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%      =  BCM5702.XpInst,     PCI\VEN_14e4&DEV_1646
%BCM5702%      =  BCM5702.XpInst,     PCI\VEN_14e4&DEV_16A6
%BCM5702%      =  BCM5702.XpInst,     PCI\VEN_14e4&DEV_16C6

[Broadcom]
%BCM5700%      =  BCM5700.Inst,     PCI\VEN_14e4&DEV_1644
%BCM5700FA%    =  BCM5700FA.Inst,   PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5700FB%    =  BCM5700FB.Inst,   PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5701%      =  BCM5701.Inst,     PCI\VEN_14e4&DEV_1645
%BCM5701FA%    =  BCM5701FA.Inst,   PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%      =  BCM5702A3.Inst,   PCI\VEN_14e4&DEV_16C6
%BCM5702%      =  BCM5702.Inst,     PCI\VEN_14e4&DEV_1646
%BCM5702%      =  BCM5702.Inst,     PCI\VEN_14e4&DEV_16A6
%BCM5703%      =  BCM5703A3.Inst,   PCI\VEN_14e4&DEV_16C7
%BCM5703%      =  BCM5703.Inst,     PCI\VEN_14e4&DEV_1647
%BCM5703%      =  BCM5703.Inst,     PCI\VEN_14e4&DEV_16A7
%BCM5703S%     =  BCM5703SA3.Inst,  PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703S%     =  BCM5703S.Inst,    PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%     =  BCM5703S.Inst,    PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703SW%    =  BCM5703SW.Inst,   PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704%      =  BCM5704.Inst,     PCI\VEN_14e4&DEV_1648
%BCM5704S%     =  BCM5704S.Inst,    PCI\VEN_14e4&DEV_16A8
%BCM5704SW%    =  BCM5704SW.Inst,   PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5705%      =  BCM5705A2.Inst,   PCI\VEN_14e4&DEV_1654
%BCM5705%      =  BCM5705A2.Inst,   PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%      =  BCM5705A2.Inst,   PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%      =  BCM5705.Inst,     PCI\VEN_14e4&DEV_1653
%BCM5705F%     =  BCM5705F.Inst,    PCI\VEN_14e4&DEV_166e
%BCM5705FHPA%  =  BCM5705F.Inst,    PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705FHPB%  =  BCM5705F.Inst,    PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%     =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e
%BCM5705M%     =  BCM5705M.Inst,    PCI\VEN_14e4&DEV_165D
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3014103c
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1658
;%BCM5750A1%   =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1676
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167A
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167B
%BCM5750A1%    =  BCM5750A1eStar.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c

%BCM5750A1%    =  BCM5750A1eStar.Inst,   PCI\VEN_14e4&DEV_165B&SUBSYS_705D103c

%BCM5750A1%    =  BCM5750A1eStar.Inst,   PCI\VEN_14e4&DEV_167A&SUBSYS_3029103c
%BCM5750A1%    =  BCM5750A1eStar.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5750A1%    =  BCM5750A1eStarAuto.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_1306103c
%BCM5750A1%    =  BCM5750A1eStarAuto.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_1307103c
%BCM5750A1%    =  BCM5750A1eStar.Inst,       PCI\VEN_14e4&DEV_167B&SUBSYS_1308103c
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_2817103c
%BCM5750A1%    =  BCM5750A1eStarAuto.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_12ff103c
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167C
%BCM5787F%     =  BCM5750A1F.Inst,  PCI\VEN_14e4&DEV_167F
%BCM5787F%     =  BCM5750A1FeStar.Inst,  PCI\VEN_14e4&DEV_167F&SUBSYS_30C0103c
%BCM5787F%     =  BCM5750A1FeStar.Inst,  PCI\VEN_14e4&DEV_167F&SUBSYS_30C2103c
%BCM5750A1%    =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_16F7
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0934103C
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0938103C
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0940103C
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0944103C
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0a0c103C
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_3095103C
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_3098103C
%BCM5750A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_3099103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_3095103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_3098103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_3099103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_309F103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30ac103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30ad103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30a3103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30a2103C
%BCM5751A1%    =  BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30b1103C
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_1658&REV_00
;%BCM5750%     =  BCM5750.Inst,     PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_167D&REV_00
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0934103C&REV0
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0938103C&REV0
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0940103C&REV0
%BCM5750%      =  BCM5750.Inst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0944103C&REV0
%BCM5787M%     =  BCM5787MeStar.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_30c0103c
%BCM5787M%     =  BCM5787MeStar.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_30c2103c
%BCM5787M%     =  BCM5787MeStar.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_30E0103c
%BCM5787M%     =  BCM5787MeStar.Inst,    PCI\VEN_14e4&DEV_169C&SUBSYS_3030103c
%BCM5787M%     =  BCM5787MeStar.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_30E3103c
%BCM5787M%     =  BCM5787MeStar.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_30DD103c
%BCM5787M%     =  BCM5787MeStar.Inst,    PCI\VEN_14e4&DEV_1693&SUBSYS_3026103c
%BCM5782%      =  BCM5782.Inst,     PCI\VEN_14e4&DEV_1696
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_099c103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_123c10cf
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_308b103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_308e103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3095103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3098103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3099103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_30aa103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_30a1103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_30b0103c
%BCM5788%      =  BCM5788.Inst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3021103c
%BCM5789%      =  BCM5789.Inst,     PCI\VEN_14e4&DEV_169d
%BCM5901%      =  BCM5901.Inst,     PCI\VEN_14e4&DEV_170D
%BCM5901%      =  BCM5901.Inst,     PCI\VEN_14e4&DEV_170e
%BCM5906%      =  BCM5906.Inst,          PCI\VEN_14e4&DEV_1712
%BCM5906%      =  BCM5906M.Inst,         PCI\VEN_14e4&DEV_1713
%BCM5906_ID4%      =  BCM5906M_ID4eStar.Inst,  PCI\VEN_14e4&DEV_1713&SUBSYS_30c0103c
%BCM5906_ID4%      =  BCM5906M_ID4eStar.Inst,  PCI\VEN_14e4&DEV_1713&SUBSYS_30c2103c
%BCM5906_ID4_FEA%  =  BCM5906_ID4_FEA.Inst, PCI\VEN_14e4&DEV_1712&SUBSYS_2816103c
%BCM5906_ID4_FEB%  =  BCM5906_ID4_FEB.Inst, PCI\VEN_14e4&DEV_1712&SUBSYS_170f103c
%BCM5906_ID4_FEA%  =  BCM5906M_ID4_FEA.Inst, PCI\VEN_14e4&DEV_1713&SUBSYS_2816103c
%BCM5906_ID4_FEB%  =  BCM5906M_ID4_FEB.Inst, PCI\VEN_14e4&DEV_1713&SUBSYS_170f103c


%OEM2_DEV1%    =  BCM5705M.Inst,    PCI\VEN_14e4&DEV_165d&SUBSYS_00580E11
%OEM2_DEV1%    =  BCM5705M.Inst,    PCI\VEN_14e4&DEV_165d&SUBSYS_005A0E11
%OEM3_DEV1%    =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0890103c
%OEM3_DEV1%    =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0a0c103c
%OEM3_DEV2%    =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0894103c
%OEM3_DEV3%    =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e&SUBSYS_088c103c
%OEM3_DEV4%    =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0727152d
%OEM3_DEV4%    =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e&SUBSYS_08bc103c
%OEM3_DEV4%    =  BCM5705MA2.Inst,  PCI\VEN_14e4&DEV_165e&SUBSYS_099c103c
%OEM3_DEV5%    =  BCM5705F.Inst,    PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3013103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3015103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_12f2103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3008103c
%OEM3_DEV6A1%  =  BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%OEM3_DEV6%    =  BCM5751.Inst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c&REV0
%OEM3_DEV6%    =  BCM5751.Inst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3002103c&REV0
%OEM3_DEV6%    =  BCM5751.Inst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c&REV0
%OEM3_DEV6%    =  BCM5751.Inst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c&REV0
%BCM5764%      =  BCM5787MeStar.Inst,         PCI\VEN_14e4&DEV_1684
%BCM5761%      =  BCM5787MeStar.Inst,         PCI\VEN_14e4&DEV_1680
%BCM5761%      =  BCM5787MeStar.Inst,         PCI\VEN_14e4&DEV_1681
%BCM5761%      =  BCM5761.Inst,               PCI\VEN_14e4&DEV_1681&SUBSYS_3047103c
%BCM5761%      =  BCM5761.Inst,               PCI\VEN_14e4&DEV_1681&SUBSYS_1459103c
%BCM5761%      =  BCM5761.Inst,               PCI\VEN_14e4&DEV_1681&SUBSYS_357E103c
%BCM5761%      =  BCM5761.Inst,               PCI\VEN_14e4&DEV_1681&SUBSYS_339C103C
[Broadcom.NTx86.5.1]
%BCM5700%      =  BCM5700CX.XpInst,   PCI\VEN_14e4&DEV_1644&REV_21
%BCM5700%      =  BCM5700CX.XpInst,   PCI\VEN_14e4&DEV_1644&REV_22
%BCM5700%      =  BCM5700.XpInst,     PCI\VEN_14e4&DEV_1644
%BCM5700FA%    =  BCM5700FA.XpInst,   PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5700FB%    =  BCM5700FB.XpInst,   PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5701%      =  BCM5701.XpInst,     PCI\VEN_14e4&DEV_1645
%BCM5701FA%    =  BCM5701FA.XpInst,   PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5702%      =  BCM5702.XpInst,     PCI\VEN_14e4&DEV_1646
%BCM5702%      =  BCM5702.XpInst,     PCI\VEN_14e4&DEV_16A6
%BCM5702%      =  BCM5702.XpInst,     PCI\VEN_14e4&DEV_16C6
%BCM5703%      =  BCM5703.XpInst,     PCI\VEN_14e4&DEV_1647
%BCM5703%      =  BCM5703.XpInst,     PCI\VEN_14e4&DEV_16A7
%BCM5703%      =  BCM5703.XpInst,     PCI\VEN_14e4&DEV_16C7
%BCM5703S%     =  BCM5703S.XpInst,    PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%     =  BCM5703S.XpInst,    PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%     =  BCM5703S.XpInst,    PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703SW%    =  BCM5703SW.XpInst,   PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704%      =  BCM5704.XpInst,     PCI\VEN_14e4&DEV_1648
%BCM5704S%     =  BCM5704S.XpInst,    PCI\VEN_14e4&DEV_16A8
%BCM5704SW%    =  BCM5704SW.XpInst,   PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5705%      =  BCM5705A2.XpInst,   PCI\VEN_14e4&DEV_1654
%BCM5705%      =  BCM5705A2.XpInst,   PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%      =  BCM5705A2.XpInst,   PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%      =  BCM5705.XpInst,     PCI\VEN_14e4&DEV_1653
%BCM5705F%     =  BCM5705F.XpInst,    PCI\VEN_14e4&DEV_166e
%BCM5705FHPA%  =  BCM5705F.XpInst,    PCI\VEN_14e4&DEV_166e&SUBSYS_1700103c
%BCM5705FHPB%  =  BCM5705F.XpInst,    PCI\VEN_14e4&DEV_166e&SUBSYS_1703103c
%BCM5705M%     =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165E
%BCM5705M%     =  BCM5705M.XpInst,    PCI\VEN_14e4&DEV_165D
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_0a0c103C
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_3095103C
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_3098103C
%BCM5750A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_3099103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_3095103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_3098103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_3099103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_309F103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30ac103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30ad103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30a3103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30a2103C
%BCM5751A1%    =  BCM5750A1M.XpInst,  PCI\VEN_14e4&DEV_16FD&SUBSYS_30b1103C
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3014103c
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_16F7
%BCM5714S%     =  BCM5714S.XpInst,    PCI\VEN_14e4&DEV_1679
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_167A
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_167B
%BCM5750A1%    =  BCM5750A1eStar.XpInst,   PCI\VEN_14e4&DEV_167B&SUBSYS_2808103c

%BCM5750A1%    =  BCM5750A1eStarX.XpInst,  PCI\VEN_14e4&DEV_165B&SUBSYS_705D103c

%BCM5750A1%    =  BCM5750A1eStar.XpInst,   PCI\VEN_14e4&DEV_167A&SUBSYS_3029103c
%BCM5750A1%    =  BCM5750A1eStar.XpInst,   PCI\VEN_14e4&DEV_167B&SUBSYS_280A103c
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_167B&SUBSYS_280C103c
%BCM5750A1%    =  BCM5750A1eStarAuto.XpInst,   PCI\VEN_14e4&DEV_167B&SUBSYS_1306103c
%BCM5750A1%    =  BCM5750A1eStarAuto.XpInst,   PCI\VEN_14e4&DEV_167B&SUBSYS_1307103c
%BCM5750A1%    =  BCM5750A1eStar.XpInst,       PCI\VEN_14e4&DEV_167B&SUBSYS_1308103c
%BCM5750A1%    =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_167B&SUBSYS_2817103c
%BCM5750A1%    =  BCM5750A1eStarAuto.XpInst,   PCI\VEN_14e4&DEV_167B&SUBSYS_12ff103c
%BCM5787F%      =  BCM5750A1F.XpInst,   PCI\VEN_14e4&DEV_167F
%BCM5787F%      =  BCM5750A1FeStar_CQ39100.XpInst,   PCI\VEN_14e4&DEV_167F&SUBSYS_30C0103c
%BCM5787F%      =  BCM5750A1FeStar_CQ39100.XpInst,   PCI\VEN_14e4&DEV_167F&SUBSYS_30C2103c
%BCM5750%      =  BCM5750.XpInst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c&REV_00
%BCM5750%      =  BCM5750.XpInst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c&REV_00
%BCM5750%      =  BCM5750.XpInst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c&REV_00
%BCM5750%      =  BCM5750.XpInst,     PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c&REV_00
%BCM5787M%   =  BCM5787MeStar_CQ39100.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_30c0103c
%BCM5787M%   =  BCM5787MeStar_CQ39100.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_30E0103c
%BCM5787M%   =  BCM5787MeStar.XpInst,         PCI\VEN_14e4&DEV_169C&SUBSYS_3030103c
%BCM5787M%   =  BCM5787MeStar_CQ39100.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_30E3103c
%BCM5787M%   =  BCM5787MeStar_CQ39100.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_30DD103c
%BCM5787M%   =  BCM5787MeStar_CQ39100.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_30c2103c
%BCM5787M%   =  BCM5787MeStar.XpInst,         PCI\VEN_14e4&DEV_1693&SUBSYS_3026103c
%BCM5782%      =  BCM5705A2.XpInst,   PCI\VEN_14e4&DEV_1696
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169C
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169C&SUBSYS_099c103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_308b103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_308e103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3095103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3098103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3099103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_30aa103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_30a1103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_30b0103c
%BCM5788%      =  BCM5788.XpInst,     PCI\VEN_14e4&DEV_169c&SUBSYS_3021103c
%BCM5789%      =  BCM5789.XpInst,     PCI\VEN_14e4&DEV_169d
%BCM5901%      =  BCM5901.XpInst,     PCI\VEN_14e4&DEV_170D
%BCM5901%      =  BCM5901.XpInst,     PCI\VEN_14e4&DEV_170E
%BCM5906%      =  BCM5906.XpInst,          PCI\VEN_14e4&DEV_1712
%BCM5906%      =  BCM5906M.XpInst,         PCI\VEN_14e4&DEV_1713
%BCM5906_ID4%      =  BCM5906M_ID4eStar.XpInst,         PCI\VEN_14e4&DEV_1713&SUBSYS_30c0103c
%BCM5906_ID4%      =  BCM5906M_ID4eStar.XpInst,         PCI\VEN_14e4&DEV_1713&SUBSYS_30c2103c
%BCM5906_ID4_FEA%  =  BCM5906_ID4_FEA.XpInst,  PCI\VEN_14e4&DEV_1712&SUBSYS_2816103c
%BCM5906_ID4_FEB%  =  BCM5906_ID4_FEB.XpInst,  PCI\VEN_14e4&DEV_1712&SUBSYS_170f103c
%BCM5906_ID4_FEA%  =  BCM5906M_ID4_FEA.XpInst, PCI\VEN_14e4&DEV_1713&SUBSYS_2816103c
%BCM5906_ID4_FEB%  =  BCM5906M_ID4_FEB.XpInst, PCI\VEN_14e4&DEV_1713&SUBSYS_170f103c

%OEM2_DEV1%    =  BCM5705M.XpInst,    PCI\VEN_14e4&DEV_165d&SUBSYS_00580E11
%OEM2_DEV1%    =  BCM5705M.XpInst,    PCI\VEN_14e4&DEV_165d&SUBSYS_005A0E11
%OEM3_DEV1%    =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0890103c
%OEM3_DEV1%    =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0a0c103c
%OEM3_DEV2%    =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0894103c
%OEM3_DEV3%    =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165e&SUBSYS_088c103c
%OEM3_DEV4%    =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165e&SUBSYS_0727152d
%OEM3_DEV4%    =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165e&SUBSYS_08bc103c
%OEM3_DEV4%    =  BCM5705MA2.XpInst,  PCI\VEN_14e4&DEV_165e&SUBSYS_099c103c
%OEM3_DEV5%    =  BCM5705F.XpInst,    PCI\VEN_14e4&DEV_166e&SUBSYS_3000103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3013103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3015103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_12f2103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3008103c
%OEM3_DEV6A1%  =  BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%OEM3_DEV6%    =  BCM5751.XpInst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c&REV_00
%OEM3_DEV6%    =  BCM5751.XpInst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3002103c&REV_00
%OEM3_DEV6%    =  BCM5751.XpInst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c&REV_00
%OEM3_DEV6%    =  BCM5751.XpInst,     PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c&REV_00

%BCM5761%      =  BCM5787MeStar.XpInst,    PCI\VEN_14e4&DEV_1680
%BCM5761%      =  BCM5787MeStar.XpInst,    PCI\VEN_14e4&DEV_1681
%BCM5761%      =  BCM5761.XpInst,          PCI\VEN_14e4&DEV_1681&SUBSYS_3047103c
%BCM5761%      =  BCM5761.XpInst,          PCI\VEN_14e4&DEV_1681&SUBSYS_1459103c
%BCM5761%      =  BCM5761.XpInst,          PCI\VEN_14e4&DEV_1681&SUBSYS_357E103c
%BCM5761%      =  BCM5761.XpInst,          PCI\VEN_14e4&DEV_1681&SUBSYS_339C103C
%BCM5764%      =  BCM5787MeStar.XpInst,    PCI\VEN_14e4&DEV_1684
%BCM5764%      =  BCM5787MeStar.XpInst,    PCI\VEN_14e4&DEV_1684&SUBSYS_1309103c
%BCM5764%      =  BCM5787MeStar.XpInst,    PCI\VEN_14e4&DEV_1684&SUBSYS_130A103c
%BCM5764%      =  BCM5787MeStar.XpInst,    PCI\VEN_14e4&DEV_1684&SUBSYS_130B103c
%BCM5764%      =  BCM5764.XpInst,          PCI\VEN_14e4&DEV_1684&SUBSYS_1503103c
%BCM5764%      =  BCM5787MeStar.XpInst,    PCI\VEN_14e4&DEV_1684&SUBSYS_2821103c

[ControlFlags]
ExcludeFromSelect = *

;*******************************************************************************
; Win2000 Install sections.
;*******************************************************************************

[BCM5700.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5700.AddService]
DisplayName    = %BCM5700%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5701.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5701.Inst.NT.Services]
AddService = b57w2k, 2, BCM5701.AddService, NtEventLog

[BCM5701.AddService]
DisplayName    = %BCM5701%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5702.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5702.Inst.NT.Services]
AddService = b57w2k, 2, BCM5702.AddService, NtEventLog

[BCM5702.AddService]
DisplayName    = %BCM5702%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5702A3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5702A3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5702A3.AddService, NtEventLog

[BCM5702A3.AddService]
DisplayName    = %BCM5702%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703.AddService, NtEventLog

[BCM5703.AddService]
DisplayName    = %BCM5703%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703A3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703A3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703A3.AddService, NtEventLog

[BCM5703A3.AddService]
DisplayName    = %BCM5703%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5704.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704.Inst.NT.Services]
AddService = b57w2k, 2, BCM5704.AddService, NtEventLog

[BCM5704.AddService]
DisplayName    = %BCM5704%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShasta, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750.AddService, NtEventLog

[BCM5750.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5789.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5789.Inst.NT.Services]
AddService = b57w2k, 2, BCM5789.AddService, NtEventLog

[BCM5789.AddService]
DisplayName    = %BCM5789%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5750A1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1.AddService, NtEventLog

[BCM5750A1.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5750A1eStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1eStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1eStar.AddService, NtEventLog

[BCM5750A1eStar.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5750A1eStarAuto.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1eStarAuto.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1eStar.AddService, NtEventLog

[BCM5750A1eStarAuto.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5750A1F.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1F.AddService, NtEventLog

[BCM5750A1F.AddService]
DisplayName    = %BCM5787F%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5750A1FeStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1FeStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1FeStar.AddService, NtEventLog

[BCM5750A1FeStar.AddService]
DisplayName    = %BCM5787F%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS




[BCM5750A1M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1M.AddService, NtEventLog

[BCM5750A1M.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5787M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5787M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5787M.AddService, NtEventLog

[BCM5787M.AddService]
DisplayName    = %BCM5787M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5761.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5761.Inst.NT.Services]
AddService = b57w2k, 2, BCM5761.AddService, NtEventLog

[BCM5761.AddService]
DisplayName    = %BCM5761%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5787MeStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5787MeStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5787MeStar.AddService, NtEventLog

[BCM5787MeStar.AddService]
DisplayName    = %BCM5787M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5906.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906.Inst.NT.Services]
AddService = b57w2k, 2, BCM5906.AddService, NtEventLog

[BCM5906.AddService]
DisplayName    = %BCM5906%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5906M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5906M.AddService, NtEventLog

[BCM5906M.AddService]
DisplayName    = %BCM5906%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5906M_ID4eStar.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906M_ID4eStar.Inst.NT.Services]
AddService = b57w2k, 2, BCM5906M_ID4eStar.AddService, NtEventLog

[BCM5906M_ID4eStar.AddService]
DisplayName    = %BCM5906_ID4%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5906_ID4_FEA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906_ID4_FEA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5906_ID4_FEA.AddService, NtEventLog

[BCM5906_ID4_FEA.AddService]
DisplayName    = %BCM5906_ID4_FEA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS




[BCM5906M_ID4_FEA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906M_ID4_FEA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5906M_ID4_FEA.AddService, NtEventLog

[BCM5906M_ID4_FEA.AddService]
DisplayName    = %BCM5906_ID4_FEA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS




[BCM5906_ID4_FEB.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906_ID4_FEB.Inst.NT.Services]
AddService = b57w2k, 2, BCM5906_ID4_FEB.AddService, NtEventLog

[BCM5906_ID4_FEB.AddService]
DisplayName    = %BCM5906_ID4_FEB%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5906M_ID4_FEB.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5906M_ID4_FEB.Inst.NT.Services]
AddService = b57w2k, 2, BCM5906M_ID4_FEB.AddService, NtEventLog

[BCM5906M_ID4_FEB.AddService]
DisplayName    = %BCM5906_ID4_FEB%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5705.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705.AddService, NtEventLog

[BCM5705.AddService]
DisplayName    = %BCM5705%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705A2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705A2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705A2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705A2.AddService, NtEventLog

[BCM5705A2.AddService]
DisplayName    = %BCM5705%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5782.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5782.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5782.Inst.NT.Services]
AddService = b57w2k, 2, BCM5782.AddService, NtEventLog

[BCM5782.AddService]
DisplayName    = %BCM5782%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5788.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5788.Inst.NT.Services]
AddService = b57w2k, 2, BCM5788.AddService, NtEventLog

[BCM5788.AddService]
DisplayName    = %BCM5788%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705M.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705M.AddService, NtEventLog

[BCM5705M.AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705MA2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705MA2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705MA2.AddService, NtEventLog

[BCM5705MA2.AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5751.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5751.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShasta
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5751.Inst.NT.Services]
AddService = b57w2k, 2, BCM5751.AddService, NtEventLog

[BCM5751.AddService]
DisplayName    = %BCM5751%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5901.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5901.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5901.Inst.NT.Services]
AddService = b57w2k, 2, BCM5901.AddService, NtEventLog

[BCM5901.AddService]
DisplayName    = %BCM5901%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705F.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705F.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705F.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705F.AddService, NtEventLog

[BCM5705F.AddService]
DisplayName    = %BCM5705F%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5700FB.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700FB.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700FB.AddService, NtEventLog

[BCM5700FB.AddService]
DisplayName    = %BCM5700FB%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5700FA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700FA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700FA.AddService, NtEventLog

[BCM5700FA.AddService]
DisplayName    = %BCM5700FA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5701FA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5701FA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5701FA.AddService, NtEventLog

[BCM5701FA.AddService]
DisplayName    = %BCM5701FA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5703S.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703S.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703S.AddService, NtEventLog

[BCM5703S.AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703SA3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703SA3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703SA3.AddService, NtEventLog

[BCM5703SA3.AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703SW.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703SW.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703SW.AddService, NtEventLog

[BCM5703SW.AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5704S.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704S.Inst.NT.Services]
AddService = b57w2k, 2, BCM5704S.AddService, NtEventLog

[BCM5704S.AddService]
DisplayName    = %BCM5704S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5704SW.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704SW.Inst.NT.Services]
AddService = b57w2k, 2, BCM5704SW.AddService, NtEventLog

[BCM5704SW.AddService]
DisplayName    = %BCM5704S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


;*******************************************************************************
; 32-bit Windows XP Install sections.
;*******************************************************************************

[BCM5700.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5700.Xp32AddService]
DisplayName    = %BCM5700%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5700CX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700CX.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700CX.Xp32AddService, Xp32EventLog

[BCM5700CX.Xp32AddService]
DisplayName    = %BCM5700%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5701.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5701.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5701.Xp32AddService, Xp32EventLog

[BCM5701.Xp32AddService]
DisplayName    = %BCM5701%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5702.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5702.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5702.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5702.Xp32AddService, Xp32EventLog

[BCM5702.Xp32AddService]
DisplayName    = %BCM5702%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5703.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5703.Xp32AddService, Xp32EventLog

[BCM5703.Xp32AddService]
DisplayName    = %BCM5703%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5704.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5704.Xp32AddService, Xp32EventLog

[BCM5704.Xp32AddService]
DisplayName    = %BCM5704%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5705.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705.Xp32AddService, Xp32EventLog

[BCM5705.Xp32AddService]
DisplayName    = %BCM5705%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5705M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705M.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705M.Xp32AddService, Xp32EventLog

[BCM5705M.Xp32AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5705F.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705F.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705F.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705F.Xp32AddService, Xp32EventLog

[BCM5705F.Xp32AddService]
DisplayName    = %BCM5705F%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5705A2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705A2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL,  ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705A2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705A2.Xp32AddService, Xp32EventLog

[BCM5705A2.Xp32AddService]
DisplayName    = %BCM5705%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5705MA2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL,  ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705MA2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705MA2.Xp32AddService, Xp32EventLog

[BCM5705MA2.Xp32AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5901.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5901.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5901.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5901.Xp32AddService, Xp32EventLog

[BCM5901.Xp32AddService]
DisplayName    = %BCM5901%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5788.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5788.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5788.Xp32AddService, Xp32EventLog

[BCM5788.Xp32AddService]
DisplayName    = %BCM5788%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5700FB.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700FB.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700FB.Xp32AddService, Xp32EventLog

[BCM5700FB.Xp32AddService]
DisplayName    = %BCM5700FB%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5700FA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700FA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700FA.Xp32AddService, Xp32EventLog

[BCM5700FA.Xp32AddService]
DisplayName    = %BCM5700FA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5701FA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5701FA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5701FA.Xp32AddService, Xp32EventLog

[BCM5701FA.Xp32AddService]
DisplayName    = %BCM5701FA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5703S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5703S.Xp32AddService, Xp32EventLog

[BCM5703S.Xp32AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5703SW.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703SW.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5703SW.Xp32AddService, Xp32EventLog

[BCM5703SW.Xp32AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5704S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5704S.Xp32AddService, Xp32EventLog

[BCM5704S.Xp32AddService]
DisplayName    = %BCM5704S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5704SW.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704SW.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5704SW.Xp32AddService, Xp32EventLog

[BCM5704SW.Xp32AddService]
DisplayName    = %BCM5704S%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5751.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5751.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL,  ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5751.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5751.Xp32AddService, Xp32EventLog

[BCM5751.Xp32AddService]
DisplayName    = %BCM5751%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5750.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShasta, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750.Xp32AddService, Xp32EventLog

[BCM5750.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5789.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5789.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5789.Xp32AddService, Xp32EventLog

[BCM5789.Xp32AddService]
DisplayName    = %BCM5789%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS




[BCM5750A1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1.Xp32AddService, Xp32EventLog

[BCM5750A1.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5750A1X.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1X.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1.Xp32AddService, Xp32EventLog

[BCM5750A1X.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5750A1eStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1eStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1eStar.Xp32AddService, Xp32EventLog

[BCM5750A1eStar.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5750A1eStarX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = Xp32AddReg, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsTuning, IntrCoal
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1eStarX.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1eStar.Xp32AddService, Xp32EventLog

[BCM5750A1eStarX.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5750A1eStarAuto.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStarAuto, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1eStarAuto.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1eStar.Xp32AddService, Xp32EventLog

[BCM5750A1eStarAuto.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1F.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1F.Xp32AddService, Xp32EventLog

[BCM5750A1F.Xp32AddService]
DisplayName    = %BCM5787F%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1FeStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1FeStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1FeStar.Xp32AddService, Xp32EventLog

[BCM5750A1FeStar.Xp32AddService]
DisplayName    = %BCM5787F%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1FeStar_CQ39100.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsCQ39100
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1FeStar_CQ39100.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1FeStar_CQ39100.Xp32AddService, Xp32EventLog

[BCM5750A1FeStar_CQ39100.Xp32AddService]
DisplayName    = %BCM5787F%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1M.Xp32AddService, Xp32EventLog

[BCM5750A1M.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5787M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5787M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5787M.Xp32AddService, Xp32EventLog

[BCM5787M.Xp32AddService]
DisplayName    = %BCM5787M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5761.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5761.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5761.Xp32AddService, Xp32EventLog

[BCM5761.Xp32AddService]
DisplayName    = %BCM5761%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5787MeStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5787MeStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5787MeStar.Xp32AddService, Xp32EventLog

[BCM5787MeStar.Xp32AddService]
DisplayName    = %BCM5787M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5787MeStar_CQ39100.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLeStar, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsCQ39100
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5787MeStar_CQ39100.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5787MeStar_CQ39100.Xp32AddService, Xp32EventLog

[BCM5787MeStar_CQ39100.Xp32AddService]
DisplayName    = %BCM5787M%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5906.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5906.Xp32AddService, Xp32EventLog

[BCM5906.Xp32AddService]
DisplayName    = %BCM5906%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5906M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5906M.Xp32AddService, Xp32EventLog

[BCM5906M.Xp32AddService]
DisplayName    = %BCM5906%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5906M_ID4eStar.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsM, ParamsCQ39100
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906M_ID4eStar.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5906M_ID4eStar.Xp32AddService, Xp32EventLog

[BCM5906M_ID4eStar.Xp32AddService]
DisplayName    = %BCM5906_ID4%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5906_ID4_FEA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906_ID4_FEA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5906_ID4_FEA.Xp32AddService, Xp32EventLog

[BCM5906_ID4_FEA.Xp32AddService]
DisplayName    = %BCM5906_ID4_FEA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS




[BCM5906M_ID4_FEA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd, DelReg.Wol
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906M_ID4_FEA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5906M_ID4_FEA.Xp32AddService, Xp32EventLog

[BCM5906M_ID4_FEA.Xp32AddService]
DisplayName    = %BCM5906_ID4_FEA%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5906_ID4_FEB.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.Wol, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906_ID4_FEB.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5906_ID4_FEB.Xp32AddService, Xp32EventLog

[BCM5906_ID4_FEB.Xp32AddService]
DisplayName    = %BCM5906_ID4_FEB%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5906M_ID4_FEB.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLeStar, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5906M_ID4_FEB.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5906M_ID4_FEB.Xp32AddService, Xp32EventLog

[BCM5906M_ID4_FEB.Xp32AddService]
DisplayName    = %BCM5906_ID4_FEB%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5764.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLeStarDefWolAuto, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5764.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5764.Xp32AddService, Xp32EventLog

[BCM5764.Xp32AddService]
DisplayName    = %BCM5764%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5714S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5750R.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsLgSndJumboCombo, ParamsTuning, IntrCoal
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5714S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog


;*******************************************************************************
; Windows NT common sections.
;*******************************************************************************

[NtAddReg]
HKR, Ndi,            Service,    0, "b57w2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[NtEventLog]
AddReg = NtAddEventLogReg

[NtAddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57w2k.sys"
HKR, , TypesSupported  , 0x00010001, 7


;*******************************************************************************
; 32-bit Windows Xp common sections.
;*******************************************************************************

[Xp32AddReg]
HKR, Ndi,            Service,    0, "b57w2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Xp32EventLog]
AddReg = Xp32AddEventLogReg

[Xp32AddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57xp32.sys"
HKR, , TypesSupported  , 0x00010001, 7



;*******************************************************************************
; Registry parameters.
;*******************************************************************************

[BCM5700.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "360"
HKR, , TxCoalescingTicks,        0, "360"
HKR, , RxMaxCoalescedFrames,     0, "15"
HKR, , TxMaxCoalescedFrames,     0, "75"


[BCM5701.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5702.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5703.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5704.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705M.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705F.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705A2.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705MA2.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5751.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5901.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5788.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5782.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750.Params]
HKR, , *TransmitBuffers,         0, "200"
HKR, , *ReceiveBuffers,          0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750R.Params]
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[ParamsNt]
HKR, Ndi\Params\TaskOffloadCap,      ParamDesc, , %TaskOffload%
HKR, Ndi\Params\TaskOffloadCap,      default,   , "63"
HKR, Ndi\Params\TaskOffloadCap,      type,      , "enum"
HKR, Ndi\Params\TaskOffloadCap\enum, 0,         , %TaskOffload_None%
HKR, Ndi\Params\TaskOffloadCap\enum, 42,        , %TaskOffload_Rx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 21,        , %TaskOffload_Tx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 63,        , %TaskOffload_Rx_Tx_Chksum%

[ParamsNT8021p]
HKR, Ndi\Params\Enable8021p,      ParamDesc, , %QOS_8021p%
HKR, Ndi\Params\Enable8021p,      default,   , "0"
HKR, Ndi\Params\Enable8021p,      type,      , "enum"
HKR, Ndi\Params\Enable8021p\enum, 0,         , %QOS_8021p_Disable%
HKR, Ndi\Params\Enable8021p\enum, 1,         , %QOS_8021p_Enable%

[ParamsNtW9x]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsJumbo]
HKR, Ndi\Params\RxMtu, ParamDesc, , %JumboMtu%
HKR, Ndi\Params\RxMtu, default,   , "1500"
HKR, Ndi\Params\RxMtu, type,      , "dword"
HKR, Ndi\Params\RxMtu, min,       , "1500"
HKR, Ndi\Params\RxMtu, max,       , "9000"
HKR, Ndi\Params\RxMtu, step,      , "500"
HKR, Ndi\Params\RxMtu, base,      , "10"

[ParamsLgSndJumboCombo]
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    ParamDesc, , %TaskOffload_LargeSend_Jumbo%
HKR, Ndi\Params\LargeSendOffloadJumboCombo,    default,   , "1"
HKR, Ndi\Params\LargeSendOffloadJumboCombo,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 0,        , %TaskOffload_LargeSend_Disable_Both%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 1,        , %TaskOffload_LargeSend_Enable_JumboDisable%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 2,        , %TaskOffload_LargeSend_Disable_JumboEnable3000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 3,        , %TaskOffload_LargeSend_Disable_JumboEnable4500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 4,        , %TaskOffload_LargeSend_Disable_JumboEnable6000%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 5,        , %TaskOffload_LargeSend_Disable_JumboEnable7500%
HKR, Ndi\Params\LargeSendOffloadJumboCombo\enum, 6,        , %TaskOffload_LargeSend_Disable_JumboEnable9000%

[ParamsWireSpeed]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%


[ParamsC]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%

[ParamsC100]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%


[ParamsWOL]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%

[ParamsWOLeStar]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "256"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%
HKR, , WolSpeed,                 0, "256"

[ParamsWOLeStarAuto]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%

[ParamsWOLShasta]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
; HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
; HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
; HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_1000mb%

[ParamsM]
HKR, , ClockControl,          0, "1"

[ParamsCQ39100]
HKR, , CQ39100,               0, "1"

[ParamsWOLTbi]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, , TbiWol,                   0, "1"

[ParamsLgSnd]
HKR, Ndi\Params\LargeSendOffload,    ParamDesc, , %TaskOffload_LargeSend%
HKR, Ndi\Params\LargeSendOffload,    default,   , "1"
HKR, Ndi\Params\LargeSendOffload,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffload\enum, 0,        , %TaskOffload_LargeSend_Disable%
HKR, Ndi\Params\LargeSendOffload\enum, 1,        , %TaskOffload_LargeSend_Enable%
HKR, , LargeSendOffload,         0, "1"

[ParamsWOLNS]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

[ParamsWOLeStarDefWolAuto]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
HKR, Ndi\Params\WolSpeed\enum,  256,       , %WolSpeed_LowestAvail%
HKR, , WolSpeed,                 0, "0"

[IntrCoal]
HKR, Ndi\Params\InterruptModeration,     ParamDesc, 0, %ParamDesc_InterruptModeration%
HKR, Ndi\Params\InterruptModeration,     Type,      0, "enum"
HKR, Ndi\Params\InterruptModeration,     Default,   0, "1"
HKR, Ndi\Params\InterruptModeration,     Optional,  0, "0"
HKR, Ndi\Params\InterruptModeration\enum, "0",      0, "%GenDisable%"
HKR, Ndi\Params\InterruptModeration\enum, "1",      0, "%GenEnable%"

[ParamsTuning]
HKR, Ndi\Params\*ReceiveBuffers,      ParamDesc,        0, %ReceiveBuffers%
HKR, Ndi\Params\*ReceiveBuffers,      type,             0, "enum"
HKR, Ndi\Params\*ReceiveBuffers,      Default,          0, "200"
HKR, Ndi\Params\*ReceiveBuffers\enum, "200",            0, "Default"
HKR, Ndi\Params\*ReceiveBuffers\enum, "16",             0, "Minimum"
HKR, Ndi\Params\*ReceiveBuffers\enum, "511",            0, "Maximum"

HKR, Ndi\Params\*TransmitBuffers,   ParamDesc,          0, %TransmitBuffers%
HKR, Ndi\Params\*TransmitBuffers,   type,               0, "int"
HKR, Ndi\Params\*TransmitBuffers,   default,            0, "200"
HKR, Ndi\Params\*TransmitBuffers,   min,                0, "100"
HKR, Ndi\Params\*TransmitBuffers,   max,                0, "600"

;*******************************************************************************
; Keys to remove.
;*******************************************************************************

[DelReg.RequestedMediaType]
HKR, Ndi\Params\RequestedMediaType

[DelReg.Wol]
HKR, Ndi\Params\WolSpeed
HKR, Ndi\Params\WakeUpModeCap

[DelReg.WolS]
HKR, Ndi\Params\WolSpeed

[DelReg.Jumbo]
HKR, Ndi\Params\RxMtu

[DelReg.LgSnd]
HKR, Ndi\Params\LargeSendOffload

[DelReg.WireSpeed]
HKR, Ndi\Params\WireSpeed

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 11
CopyFile.XpSys32 = 12
CopyFile.NtSys  = 12

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
b57xp32.sys = 1
b57w2k.sys = 1

[CopyFile.XpSys32]
b57xp32.sys,,,1

[CopyFile.NtSys]
b57w2k.sys,,,1


;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
BRCM                = "Broadcom"
DISK_DESC           = "Broadcom NetXtreme Installation Media"

BCM5700             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5701             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5702             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705F            = "Broadcom 570x 10/100 Integrated Controller"
BCM5901             = "Broadcom NetXtreme Fast Ethernet"
BCM5782             = "Broadcom NetXtreme Gigabit Ethernet for hp"
BCM5761             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5764             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5787M            = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5787F            = "Broadcom NetLink (TM) Fast Ethernet"
BCM5788             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5789             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5906             = "Broadcom NetLink (TM) Fast Ethernet"
BCM5906_ID4         = "Broadcom 590x 10/100 Ethernet"
BCM5750             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5751             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5751A1           = "Broadcom NetXtreme Gigabit Ethernet"

BCM5700FB           = "Broadcom NetXtreme Gigabit Fiber"
BCM5700FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5703S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5703SW           = "Broadcom NetXtreme Gigabit Fiber WOL"
BCM5704S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5714S            = "Broadcom NetXtreme Gigabit Fiber"

OEM2_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV4           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV5           = "Broadcom 570x 10/100 Integrated Controller"
OEM3_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV6A1         = "Broadcom NetXtreme Gigabit Ethernet"

BCM5705FHPA         = "Broadcom NetXtreme FE-A"
BCM5705FHPB         = "Broadcom NetXtreme FE-B"

BCM5906_ID4_FEA     = "Broadcom NetLink (TM) FE-A"
BCM5906_ID4_FEB     = "Broadcom NetLink (TM) FE-B"

JumboMtu = "Jumbo Mtu"

FlowControl             = "Flow Control"
FlowControl_Disable     = "Disable"
FlowControl_Rx_Pause    = "Rx PAUSE"
FlowControl_Tx_Pause    = "Tx PAUSE"
FlowControl_Rx_Tx_Pause = "Rx/Tx PAUSE"
FlowControl_Auto        = "Auto"

Speed_Duplex          = "Speed & Duplex"
Speed_Duplex_Auto     = "Auto"
Speed_Duplex_10Mb_Hd  = "10 Mb Half"
Speed_Duplex_10Mb_Fd  = "10 Mb Full"
Speed_Duplex_100Mb_Hd = "100 Mb Half"
Speed_Duplex_100Mb_Fd = "100 Mb Full"
Speed_Duplex_1000Mb_Fd = "1000 Mb Full"

QOS_8021p         = "802.1p QOS"
QOS_8021p_Disable = "Disable"
QOS_8021p_Enable  = "Enable"

WireSpeed         = "Ethernet@WireSpeed"
WireSpeed_Disable = "Disable"
WireSpeed_Enable  = "Enable"

TaskOffload              = "Checksum Offload"
TaskOffload_None         = "None"
TaskOffload_Rx_Chksum    = "Rx TCP/IP Checksum"
TaskOffload_Tx_Chksum    = "Tx TCP/IP Checksum"
TaskOffload_Rx_Tx_Chksum = "Tx/Rx TCP/IP Checksum"

TaskOffload_LargeSend           = "Large Send Offload"
TaskOffload_LargeSend_Disable   = "Disable"
TaskOffload_LargeSend_Enable    = "Enable"

TaskOffload_LargeSend_Jumbo                           = "LSO & Jumbo Frames"
TaskOffload_LargeSend_Disable_Both                = "Both Disabled"
TaskOffload_LargeSend_Enable_JumboDisable   = "LSO Enabled,Jumbo Off"
TaskOffload_LargeSend_Disable_JumboEnable3000   = "LSO Off,Jumbo 3000"
TaskOffload_LargeSend_Disable_JumboEnable4500   = "LSO Off,Jumbo 4500"
TaskOffload_LargeSend_Disable_JumboEnable6000   = "LSO Off,Jumbo 6000"
TaskOffload_LargeSend_Disable_JumboEnable7500   = "LSO Off,Jumbo 7500"
TaskOffload_LargeSend_Disable_JumboEnable9000   = "LSO Off,Jumbo 9000"

WakeUpMode         = "Wake Up Capabilities"
WakeUpMode_None    = "None"
WakeUpMode_Magic   = "Magic Packet"
WakeUpMode_Pattern = "Wake Up Frame"
WakeUpMode_Both    = "Both"

WolSpeed       = "WOL Speed"
WolSpeed_Auto  = "Auto"
WolSpeed_10mb  = "10 Mb"
WolSpeed_100mb = "100 Mb"
WolSpeed_1000mb = "1000 Mb"
WolSpeed_LowestAvail = "Lowest Speed Advertised"

NetworkAddress           = "Locally Administered Address"

ParamDesc_InterruptModeration   = "Interrupt Moderation"
ReceiveBuffers  =       "Receive Buffers"
TransmitBuffers =       "Transmit Buffers"

;; Interrupt Coalescing Options
;;
GenEnable       = "Enable"
GenDisable      = "Disable"


